/*
 * Device Tree Source for IGEPv2 Rev. (TI OMAP AM/DM37x)
 *
 * Copyright (C) 2012 Javier Martinez Canillas <javier@collabora.co.uk>
 * Copyright (C) 2012 Enric Balletbo i Serra <eballetbo@gmail.com>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

#include "omap3-igep.dtsi"
#include "omap-gpmc-smsc911x.dtsi"

/ {
	model = "IGEPv2 (TI OMAP AM/DM37x)";
	compatible = "isee,omap3-igep0020", "ti,omap36xx", "ti,omap3";

	leds {
		pinctrl-names = "default";
		pinctrl-0 = <&leds_pins>;
		compatible = "gpio-leds";

		boot {
			 label = "omap3:green:boot";
			 gpios = <&gpio1 26 GPIO_ACTIVE_HIGH>;
			 default-state = "on";
		};

		user0 {
			 label = "omap3:red:user0";
			 gpios = <&gpio1 27 GPIO_ACTIVE_HIGH>;
			 default-state = "off";
		};

		user1 {
			 label = "omap3:red:user1";
			 gpios = <&gpio1 28 GPIO_ACTIVE_HIGH>;
			 default-state = "off";
		};

		user2 {
			label = "omap3:green:user1";
			gpios = <&twl_gpio 19 GPIO_ACTIVE_LOW>;
		};
	};

       /* HS USB Port 1 Power */
       hsusb1_power: hsusb1_power_reg {
               compatible = "regulator-fixed";
               regulator-name = "hsusb1_vbus";
               regulator-min-microvolt = <3300000>;
               regulator-max-microvolt = <3300000>;
               gpio = <&twl_gpio 18 GPIO_ACTIVE_LOW>;	/* GPIO LEDA */
               startup-delay-us = <70000>;
       };

	/* HS USB Host PHY on PORT 1 */
	hsusb1_phy: hsusb1_phy {
		compatible = "usb-nop-xceiv";
		reset-gpios = <&gpio1 24 GPIO_ACTIVE_LOW>; /* gpio_24 */
		vcc-supply = <&hsusb1_power>;
	};

	tfp410: encoder@0 {
		compatible = "ti,tfp410";
		powerdown-gpios = <&gpio6 10 GPIO_ACTIVE_LOW>; /* gpio_170 */

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				tfp410_in: endpoint@0 {
					remote-endpoint = <&dpi_out>;
				};
			};

			port@1 {
				reg = <1>;

				tfp410_out: endpoint@0 {
					remote-endpoint = <&dvi_connector_in>;
				};
			};
		};
	};

	dvi0: connector@0 {
		compatible = "dvi-connector";
		label = "dvi";

		digital;

		ddc-i2c-bus = <&i2c3>;

		port {
			dvi_connector_in: endpoint {
				remote-endpoint = <&tfp410_out>;
			};
		};
	};
};

&omap3_pmx_core {
	pinctrl-names = "default";
	pinctrl-0 = <
		&tfp410_pins
		&dss_dpi_pins
	>;

	tfp410_pins: pinmux_tfp410_pins {
		pinctrl-single,pins = <
			0x196 (PIN_OUTPUT | MUX_MODE4)   /* hdq_sio.gpio_170 */
		>;
	};

	dss_dpi_pins: pinmux_dss_dpi_pins {
		pinctrl-single,pins = <
			0x0a4 (PIN_OUTPUT | MUX_MODE0)   /* dss_pclk.dss_pclk */
			0x0a6 (PIN_OUTPUT | MUX_MODE0)   /* dss_hsync.dss_hsync */
			0x0a8 (PIN_OUTPUT | MUX_MODE0)   /* dss_vsync.dss_vsync */
			0x0aa (PIN_OUTPUT | MUX_MODE0)   /* dss_acbias.dss_acbias */
			0x0ac (PIN_OUTPUT | MUX_MODE0)   /* dss_data0.dss_data0 */
			0x0ae (PIN_OUTPUT | MUX_MODE0)   /* dss_data1.dss_data1 */
			0x0b0 (PIN_OUTPUT | MUX_MODE0)   /* dss_data2.dss_data2 */
			0x0b2 (PIN_OUTPUT | MUX_MODE0)   /* dss_data3.dss_data3 */
			0x0b4 (PIN_OUTPUT | MUX_MODE0)   /* dss_data4.dss_data4 */
			0x0b6 (PIN_OUTPUT | MUX_MODE0)   /* dss_data5.dss_data5 */
			0x0b8 (PIN_OUTPUT | MUX_MODE0)   /* dss_data6.dss_data6 */
			0x0ba (PIN_OUTPUT | MUX_MODE0)   /* dss_data7.dss_data7 */
			0x0bc (PIN_OUTPUT | MUX_MODE0)   /* dss_data8.dss_data8 */
			0x0be (PIN_OUTPUT | MUX_MODE0)   /* dss_data9.dss_data9 */
			0x0c0 (PIN_OUTPUT | MUX_MODE0)   /* dss_data10.dss_data10 */
			0x0c2 (PIN_OUTPUT | MUX_MODE0)   /* dss_data11.dss_data11 */
			0x0c4 (PIN_OUTPUT | MUX_MODE0)   /* dss_data12.dss_data12 */
			0x0c6 (PIN_OUTPUT | MUX_MODE0)   /* dss_data13.dss_data13 */
			0x0c8 (PIN_OUTPUT | MUX_MODE0)   /* dss_data14.dss_data14 */
			0x0ca (PIN_OUTPUT | MUX_MODE0)   /* dss_data15.dss_data15 */
			0x0cc (PIN_OUTPUT | MUX_MODE0)   /* dss_data16.dss_data16 */
			0x0ce (PIN_OUTPUT | MUX_MODE0)   /* dss_data17.dss_data17 */
			0x0d0 (PIN_OUTPUT | MUX_MODE0)   /* dss_data18.dss_data18 */
			0x0d2 (PIN_OUTPUT | MUX_MODE0)   /* dss_data19.dss_data19 */
			0x0d4 (PIN_OUTPUT | MUX_MODE0)   /* dss_data20.dss_data20 */
			0x0d6 (PIN_OUTPUT | MUX_MODE0)   /* dss_data21.dss_data21 */
			0x0d8 (PIN_OUTPUT | MUX_MODE0)   /* dss_data22.dss_data22 */
			0x0da (PIN_OUTPUT | MUX_MODE0)   /* dss_data23.dss_data23 */
		>;
	};
};

&omap3_pmx_core2 {
	pinctrl-names = "default";
	pinctrl-0 = <
		&hsusbb1_pins
	>;

	hsusbb1_pins: pinmux_hsusbb1_pins {
		pinctrl-single,pins = <
			OMAP3630_CORE2_IOPAD(0x25da, PIN_OUTPUT | MUX_MODE3)		/* etk_ctl.hsusb1_clk */
			OMAP3630_CORE2_IOPAD(0x25d8, PIN_OUTPUT | MUX_MODE3)		/* etk_clk.hsusb1_stp */
			OMAP3630_CORE2_IOPAD(0x25ec, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d8.hsusb1_dir */
			OMAP3630_CORE2_IOPAD(0x25ee, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d9.hsusb1_nxt */
			OMAP3630_CORE2_IOPAD(0x25dc, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d0.hsusb1_data0 */
			OMAP3630_CORE2_IOPAD(0x25de, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d1.hsusb1_data1 */
			OMAP3630_CORE2_IOPAD(0x25e0, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d2.hsusb1_data2 */
			OMAP3630_CORE2_IOPAD(0x25e2, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d3.hsusb1_data7 */
			OMAP3630_CORE2_IOPAD(0x25e4, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d4.hsusb1_data4 */
			OMAP3630_CORE2_IOPAD(0x25e6, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d5.hsusb1_data5 */
			OMAP3630_CORE2_IOPAD(0x25e8, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d6.hsusb1_data6 */
			OMAP3630_CORE2_IOPAD(0x25ea, PIN_INPUT_PULLDOWN | MUX_MODE3)	/* etk_d7.hsusb1_data3 */
		>;
	};

	leds_pins: pinmux_leds_pins {
		pinctrl-single,pins = <
			OMAP3630_CORE2_IOPAD(0x25f4, PIN_OUTPUT | MUX_MODE4) /* etk_d12.gpio_26 */
			OMAP3630_CORE2_IOPAD(0x25f6, PIN_OUTPUT | MUX_MODE4) /* etk_d13.gpio_27 */
			OMAP3630_CORE2_IOPAD(0x25f8, PIN_OUTPUT | MUX_MODE4) /* etk_d14.gpio_28 */
		>;
	};
};

&i2c3 {
	clock-frequency = <100000>;

	/*
	 * Display monitor features are burnt in the EEPROM
	 * as EDID data.
	 */
	eeprom@50 {
		compatible = "ti,eeprom";
		reg = <0x50>;
	};
};

&gpmc {
	ranges = <0 0 0x00000000 0x20000000>,
		 <5 0 0x2c000000 0x01000000>;

	nand@0,0 {
		linux,mtd-name= "micron,mt29c4g96maz";
		reg = <0 0 0>;
		nand-bus-width = <16>;
		ti,nand-ecc-opt = "bch8";

		gpmc,sync-clk-ps = <0>;
		gpmc,cs-on-ns = <0>;
		gpmc,cs-rd-off-ns = <44>;
		gpmc,cs-wr-off-ns = <44>;
		gpmc,adv-on-ns = <6>;
		gpmc,adv-rd-off-ns = <34>;
		gpmc,adv-wr-off-ns = <44>;
		gpmc,we-off-ns = <40>;
		gpmc,oe-off-ns = <54>;
		gpmc,access-ns = <64>;
		gpmc,rd-cycle-ns = <82>;
		gpmc,wr-cycle-ns = <82>;
		gpmc,wr-access-ns = <40>;
		gpmc,wr-data-mux-bus-ns = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "SPL";
			reg = <0 0x100000>;
		};
		partition@80000 {
			label = "U-Boot";
			reg = <0x100000 0x180000>;
		};
		partition@1c0000 {
			label = "Environment";
			reg = <0x280000 0x100000>;
		};
		partition@280000 {
			label = "Kernel";
			reg = <0x380000 0x300000>;
		};
		partition@780000 {
			label = "Filesystem";
			reg = <0x680000 0x1f980000>;
		};
	};

	ethernet@gpmc {
		pinctrl-names = "default";
		pinctrl-0 = <&smsc911x_pins>;
		reg = <5 0 0xff>;
		interrupt-parent = <&gpio6>;
		interrupts = <16 IRQ_TYPE_LEVEL_LOW>;
	};
};

&usbhshost {
	port1-mode = "ehci-phy";
};

&usbhsehci {
	phys = <&hsusb1_phy>;
};

&vpll2 {
        /* Needed for DSS */
        regulator-name = "vdds_dsi";
};

&dss {
	status = "ok";

	port {
		dpi_out: endpoint {
			remote-endpoint = <&tfp410_in>;
			data-lines = <24>;
		};
	};
};
