/*
 * Copyright 2013 CompuLab Ltd.
 *
 * Author: Valentin Raevsky <valentin@compulab.co.il>
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
#include "imx6q.dtsi"

/ {
	model = "CompuLab CM-FX6";
	compatible = "compulab,cm-fx6", "fsl,imx6q";

	memory {
		reg = <0x10000000 0x80000000>;
	};

	leds {
		compatible = "gpio-leds";

		heartbeat-led {
			label = "Heartbeat";
			gpios = <&gpio2 31 0>;
			linux,default-trigger = "heartbeat";
		};
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	status = "okay";
};

&gpmi {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpmi_nand>;
	status = "okay";
};

&iomuxc {
	imx6q-cm-fx6 {
		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
				MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
			>;
		};

		pinctrl_gpmi_nand: gpminandgrp {
			fsl,pins = <
				MX6QDL_PAD_NANDF_CLE__NAND_CLE		0xb0b1
				MX6QDL_PAD_NANDF_ALE__NAND_ALE		0xb0b1
				MX6QDL_PAD_NANDF_WP_B__NAND_WP_B	0xb0b1
				MX6QDL_PAD_NANDF_RB0__NAND_READY_B	0xb000
				MX6QDL_PAD_NANDF_CS0__NAND_CE0_B	0xb0b1
				MX6QDL_PAD_NANDF_CS1__NAND_CE1_B	0xb0b1
				MX6QDL_PAD_SD4_CMD__NAND_RE_B		0xb0b1
				MX6QDL_PAD_SD4_CLK__NAND_WE_B		0xb0b1
				MX6QDL_PAD_NANDF_D0__NAND_DATA00	0xb0b1
				MX6QDL_PAD_NANDF_D1__NAND_DATA01	0xb0b1
				MX6QDL_PAD_NANDF_D2__NAND_DATA02	0xb0b1
				MX6QDL_PAD_NANDF_D3__NAND_DATA03	0xb0b1
				MX6QDL_PAD_NANDF_D4__NAND_DATA04	0xb0b1
				MX6QDL_PAD_NANDF_D5__NAND_DATA05	0xb0b1
				MX6QDL_PAD_NANDF_D6__NAND_DATA06	0xb0b1
				MX6QDL_PAD_NANDF_D7__NAND_DATA07	0xb0b1
				MX6QDL_PAD_SD4_DAT0__NAND_DQS		0x00b1
			>;
		};

		pinctrl_uart4: uart4grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL0__UART4_TX_DATA	0x1b0b1
				MX6QDL_PAD_KEY_ROW0__UART4_RX_DATA	0x1b0b1
			>;
		};
	};
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
	status = "okay";
};
