/*
 * wm8750.dtsi - Device tree file for Wondermedia WM8750 SoC
 *
 * Copyright (C) 2012 Tony Prisk <linux@prisktech.co.nz>
 *
 * Licensed under GPLv2 or later
 */

/include/ "skeleton.dtsi"

/ {
	compatible = "wm,wm8750";

	cpus {
		#address-cells = <0>;
		#size-cells = <0>;

		cpu {
			device_type = "cpu";
			compatible = "arm,arm1176ej-s";
		};
	};

	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		i2c0 = &i2c_0;
		i2c1 = &i2c_1;
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		ranges;
		interrupt-parent = <&intc0>;

		intc0: interrupt-controller@d8140000 {
			compatible = "via,vt8500-intc";
			interrupt-controller;
			reg = <0xd8140000 0x10000>;
			#interrupt-cells = <1>;
		};

		/* Secondary IC cascaded to intc0 */
		intc1: interrupt-controller@d8150000 {
			compatible = "via,vt8500-intc";
			interrupt-controller;
			#interrupt-cells = <1>;
			reg = <0xD8150000 0x10000>;
			interrupts = <56 57 58 59 60 61 62 63>;
		};

		pinctrl: pinctrl@d8110000 {
			compatible = "wm,wm8750-pinctrl";
			reg = <0xd8110000 0x10000>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		pmc@d8130000 {
			compatible = "via,vt8500-pmc";
			reg = <0xd8130000 0x1000>;

			clocks {
				#address-cells = <1>;
				#size-cells = <0>;

				ref24: ref24M {
					#clock-cells = <0>;
					compatible = "fixed-clock";
					clock-frequency = <24000000>;
				};

				ref25: ref25M {
					#clock-cells = <0>;
					compatible = "fixed-clock";
					clock-frequency = <25000000>;
				};

				plla: plla {
					#clock-cells = <0>;
					compatible = "wm,wm8750-pll-clock";
					clocks = <&ref25>;
					reg = <0x200>;
				};

				pllb: pllb {
					#clock-cells = <0>;
					compatible = "wm,wm8750-pll-clock";
					clocks = <&ref25>;
					reg = <0x204>;
				};

				pllc: pllc {
					#clock-cells = <0>;
					compatible = "wm,wm8750-pll-clock";
					clocks = <&ref25>;
					reg = <0x208>;
				};

				plld: plld {
					#clock-cells = <0>;
					compatible = "wm,wm8750-pll-clock";
					clocks = <&ref25>;
					reg = <0x20C>;
				};

				plle: plle {
					#clock-cells = <0>;
					compatible = "wm,wm8750-pll-clock";
					clocks = <&ref25>;
					reg = <0x210>;
				};

				clkarm: arm {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&plla>;
					divisor-reg = <0x300>;
				};

				clkahb: ahb {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x304>;
				};

				clkapb: apb {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x320>;
				};

				clkddr: ddr {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&plld>;
					divisor-reg = <0x310>;
				};

				clkuart0: uart0 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x254>;
					enable-bit = <24>;
				};

				clkuart1: uart1 {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&ref24>;
					enable-reg = <0x254>;
					enable-bit = <25>;
				};

                                clkuart2: uart2 {
                                        #clock-cells = <0>;
                                        compatible = "via,vt8500-device-clock";
                                        clocks = <&ref24>;
                                        enable-reg = <0x254>;
                                        enable-bit = <26>;
                                };

                                clkuart3: uart3 {
                                        #clock-cells = <0>;
                                        compatible = "via,vt8500-device-clock";
                                        clocks = <&ref24>;
                                        enable-reg = <0x254>;
                                        enable-bit = <27>;
                                };

                                clkuart4: uart4 {
                                        #clock-cells = <0>;
                                        compatible = "via,vt8500-device-clock";
                                        clocks = <&ref24>;
                                        enable-reg = <0x254>;
                                        enable-bit = <28>;
                                };

                                clkuart5: uart5 {
                                        #clock-cells = <0>;
                                        compatible = "via,vt8500-device-clock";
                                        clocks = <&ref24>;
                                        enable-reg = <0x254>;
                                        enable-bit = <29>;
                                };

				clkpwm: pwm {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x350>;
					enable-reg = <0x250>;
					enable-bit = <17>;
				};

				clksdhc: sdhc {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x330>;
					divisor-mask = <0x3f>;
					enable-reg = <0x250>;
					enable-bit = <0>;
				};

				clki2c0: i2c0clk {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x3A0>;
					enable-reg = <0x250>;
					enable-bit = <8>;
				};

				clki2c1: i2c1clk {
					#clock-cells = <0>;
					compatible = "via,vt8500-device-clock";
					clocks = <&pllb>;
					divisor-reg = <0x3A4>;
					enable-reg = <0x250>;
					enable-bit = <9>;
				};
			};
		};

		pwm: pwm@d8220000 {
			#pwm-cells = <3>;
			compatible = "via,vt8500-pwm";
			reg = <0xd8220000 0x100>;
			clocks = <&clkpwm>;
		};

		timer@d8130100 {
			compatible = "via,vt8500-timer";
			reg = <0xd8130100 0x28>;
			interrupts = <36>;
		};

		ehci@d8007900 {
			compatible = "via,vt8500-ehci";
			reg = <0xd8007900 0x200>;
			interrupts = <26>;
		};

		uhci@d8007b00 {
			compatible = "platform-uhci";
			reg = <0xd8007b00 0x200>;
			interrupts = <26>;
		};

		uhci@d8008d00 {
			compatible = "platform-uhci";
			reg = <0xd8008d00 0x200>;
			interrupts = <26>;
		};

		uart0: serial@d8200000 {
			compatible = "via,vt8500-uart";
			reg = <0xd8200000 0x1040>;
			interrupts = <32>;
			clocks = <&clkuart0>;
			status = "disabled";
		};

		uart1: serial@d82b0000 {
			compatible = "via,vt8500-uart";
			reg = <0xd82b0000 0x1040>;
			interrupts = <33>;
			clocks = <&clkuart1>;
			status = "disabled";
		};

                uart2: serial@d8210000 {
                        compatible = "via,vt8500-uart";
                        reg = <0xd8210000 0x1040>;
                        interrupts = <47>;
                        clocks = <&clkuart2>;
			status = "disabled";
                };

                uart3: serial@d82c0000 {
                        compatible = "via,vt8500-uart";
                        reg = <0xd82c0000 0x1040>;
                        interrupts = <50>;
                        clocks = <&clkuart3>;
			status = "disabled";
                };

                uart4: serial@d8370000 {
                        compatible = "via,vt8500-uart";
                        reg = <0xd8370000 0x1040>;
                        interrupts = <30>;
                        clocks = <&clkuart4>;
			status = "disabled";
                };

                uart5: serial@d8380000 {
                        compatible = "via,vt8500-uart";
                        reg = <0xd8380000 0x1040>;
                        interrupts = <43>;
                        clocks = <&clkuart5>;
			status = "disabled";
                };

		rtc@d8100000 {
			compatible = "via,vt8500-rtc";
			reg = <0xd8100000 0x10000>;
			interrupts = <48>;
		};

		sdhc@d800a000 {
			compatible = "wm,wm8505-sdhc";
			reg = <0xd800a000 0x1000>;
			interrupts = <20 21>;
			clocks = <&clksdhc>;
			bus-width = <4>;
			sdon-inverted;
		};

		i2c_0: i2c@d8280000 {
			compatible = "wm,wm8505-i2c";
			reg = <0xd8280000 0x1000>;
			interrupts = <19>;
			clocks = <&clki2c0>;
			clock-frequency = <400000>;
		};

		i2c_1: i2c@d8320000 {
			compatible = "wm,wm8505-i2c";
			reg = <0xd8320000 0x1000>;
			interrupts = <18>;
			clocks = <&clki2c1>;
			clock-frequency = <400000>;
		};
	};
};
