/*
 * Copyright 2013 Crystalfontz America, Inc.
 * Copyright 2013 Free Electrons
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/*
 * The CFA-10058 is an expansion board for the CFA-10036 module, thus we
 * need to include the CFA-10036 DTS.
 */
#include "imx28-cfa10036.dts"

/ {
	model = "Crystalfontz CFA-10058 Board";
	compatible = "crystalfontz,cfa10058", "crystalfontz,cfa10036", "fsl,imx28";

	apb@80000000 {
		apbh@80000000 {
			pinctrl@80018000 {
				usb_pins_cfa10058: usb-10058@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						MX28_PAD_GPMI_D07__GPIO_0_7
					>;
					fsl,drive-strength = <MXS_DRIVE_4mA>;
					fsl,voltage = <MXS_VOLTAGE_HIGH>;
					fsl,pull-up = <MXS_PULL_DISABLE>;
				};

				lcdif_pins_cfa10058: lcdif-10058@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						MX28_PAD_LCD_RD_E__LCD_VSYNC
						MX28_PAD_LCD_WR_RWN__LCD_HSYNC
						MX28_PAD_LCD_RS__LCD_DOTCLK
						MX28_PAD_LCD_CS__LCD_ENABLE
					>;
					fsl,drive-strength = <MXS_DRIVE_4mA>;
					fsl,voltage = <MXS_VOLTAGE_HIGH>;
					fsl,pull-up = <MXS_PULL_DISABLE>;
				};
			};

			lcdif@80030000 {
				pinctrl-names = "default";
				pinctrl-0 = <&lcdif_24bit_pins_a
						 &lcdif_pins_cfa10058>;
				display = <&display>;
				status = "okay";

				display: display {
					bits-per-pixel = <32>;
					bus-width = <24>;

					display-timings {
						native-mode = <&timing0>;
						timing0: timing0 {
							clock-frequency = <30000000>;
							hactive = <800>;
							vactive = <480>;
							hback-porch = <40>;
							hfront-porch = <40>;
							vback-porch = <13>;
							vfront-porch = <29>;
							hsync-len = <8>;
							vsync-len = <8>;
							hsync-active = <0>;
							vsync-active = <0>;
							de-active = <1>;
							pixelclk-active = <1>;
						};
					};
				};
			};
		};

		apbx@80040000 {
			lradc@80050000 {
				fsl,lradc-touchscreen-wires = <4>;
				status = "okay";
			};

			pwm: pwm@80064000 {
				pinctrl-names = "default";
				pinctrl-0 = <&pwm3_pins_b>;
				status = "okay";
			};

			usbphy1: usbphy@8007e000 {
				status = "okay";
			};
		};
	};

	ahb@80080000 {
		usb1: usb@80090000 {
			vbus-supply = <&reg_usb1_vbus>;
			pinctrl-0 = <&usb1_pins_a>;
			pinctrl-names = "default";
			status = "okay";
		};
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_usb1_vbus: regulator@0 {
			pinctrl-names = "default";
			pinctrl-0 = <&usb_pins_cfa10058>;
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "usb1_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio0 7 1>;
		};
	};

	ahb@80080000 {
		mac0: ethernet@800f0000 {
			phy-mode = "rmii";
			pinctrl-names = "default";
			pinctrl-0 = <&mac0_pins_a>;
			phy-reset-gpios = <&gpio2 21 0>;
			phy-reset-duration = <100>;
			status = "okay";
		};
	};

	backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm 3 5000000>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <6>;
	};
};
