/*
 * Copyright (c) 2013 MundoReader S.L.
 * Author: Heiko Stuebner <heiko@sntech.de>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation; either version 2 of the License, or
 * (at your option) any later version.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include "skeleton.dtsi"

/ {
	interrupt-parent = <&gic>;

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		ranges;

		scu@1013c000 {
			compatible = "arm,cortex-a9-scu";
			reg = <0x1013c000 0x100>;
		};

		pmu@20004000 {
			compatible = "rockchip,rk3066-pmu";
			reg = <0x20004000 0x100>;
		};

		gic: interrupt-controller@1013d000 {
			compatible = "arm,cortex-a9-gic";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x1013d000 0x1000>,
			      <0x1013c100 0x0100>;
		};

		L2: l2-cache-controller@10138000 {
			compatible = "arm,pl310-cache";
			reg = <0x10138000 0x1000>;
			cache-unified;
			cache-level = <2>;
		};

		global-timer@1013c200 {
			compatible = "arm,cortex-a9-global-timer";
			reg = <0x1013c200 0x20>;
			interrupts = <GIC_PPI 11 0x304>;
			clocks = <&dummy150m>;
		};

		local-timer@1013c600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0x1013c600 0x20>;
			interrupts = <GIC_PPI 13 0x304>;
			clocks = <&dummy150m>;
		};

		uart0: serial@10124000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x10124000 0x400>;
			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <1>;
			clocks = <&clk_gates1 8>;
			status = "disabled";
		};

		uart1: serial@10126000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x10126000 0x400>;
			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <1>;
			clocks = <&clk_gates1 10>;
			status = "disabled";
		};

		uart2: serial@20064000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x20064000 0x400>;
			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <1>;
			clocks = <&clk_gates1 12>;
			status = "disabled";
		};

		uart3: serial@20068000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x20068000 0x400>;
			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <1>;
			clocks = <&clk_gates1 14>;
			status = "disabled";
		};

		dwmmc@10214000 {
			compatible = "rockchip,rk2928-dw-mshc";
			reg = <0x10214000 0x1000>;
			interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;

			clocks = <&clk_gates5 10>, <&clk_gates2 11>;
			clock-names = "biu", "ciu";

			status = "disabled";
		};

		dwmmc@10218000 {
			compatible = "rockchip,rk2928-dw-mshc";
			reg = <0x10218000 0x1000>;
			interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;

			clocks = <&clk_gates5 11>, <&clk_gates2 13>;
			clock-names = "biu", "ciu";

			status = "disabled";
		};
	};
};
