/*
 * at91sam9x5.dtsi - Device Tree Include file for AT91SAM9x5 family SoC
 *                   applies to AT91SAM9G15, AT91SAM9G25, AT91SAM9G35,
 *                   AT91SAM9X25, AT91SAM9X35 SoC
 *
 *  Copyright (C) 2012 Atmel,
 *                2012 Nicolas Ferre <nicolas.ferre@atmel.com>
 *
 * Licensed under GPLv2 or later.
 */

#include "skeleton.dtsi"
#include <dt-bindings/dma/at91.h>
#include <dt-bindings/pinctrl/at91.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	model = "Atmel AT91SAM9x5 family SoC";
	compatible = "atmel,at91sam9x5";
	interrupt-parent = <&aic>;

	aliases {
		serial0 = &dbgu;
		serial1 = &usart0;
		serial2 = &usart1;
		serial3 = &usart2;
		gpio0 = &pioA;
		gpio1 = &pioB;
		gpio2 = &pioC;
		gpio3 = &pioD;
		tcb0 = &tcb0;
		tcb1 = &tcb1;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		ssc0 = &ssc0;
		pwm0 = &pwm0;
	};
	cpus {
		#address-cells = <0>;
		#size-cells = <0>;

		cpu {
			compatible = "arm,arm926ej-s";
			device_type = "cpu";
		};
	};

	memory {
		reg = <0x20000000 0x10000000>;
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			aic: interrupt-controller@fffff000 {
				#interrupt-cells = <3>;
				compatible = "atmel,at91rm9200-aic";
				interrupt-controller;
				reg = <0xfffff000 0x200>;
				atmel,external-irqs = <31>;
			};

			ramc0: ramc@ffffe800 {
				compatible = "atmel,at91sam9g45-ddramc";
				reg = <0xffffe800 0x200>;
			};

			pmc: pmc@fffffc00 {
				compatible = "atmel,at91rm9200-pmc";
				reg = <0xfffffc00 0x100>;
			};

			rstc@fffffe00 {
				compatible = "atmel,at91sam9g45-rstc";
				reg = <0xfffffe00 0x10>;
			};

			shdwc@fffffe10 {
				compatible = "atmel,at91sam9x5-shdwc";
				reg = <0xfffffe10 0x10>;
			};

			pit: timer@fffffe30 {
				compatible = "atmel,at91sam9260-pit";
				reg = <0xfffffe30 0xf>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
			};

			tcb0: timer@f8008000 {
				compatible = "atmel,at91sam9x5-tcb";
				reg = <0xf8008000 0x100>;
				interrupts = <17 IRQ_TYPE_LEVEL_HIGH 0>;
			};

			tcb1: timer@f800c000 {
				compatible = "atmel,at91sam9x5-tcb";
				reg = <0xf800c000 0x100>;
				interrupts = <17 IRQ_TYPE_LEVEL_HIGH 0>;
			};

			dma0: dma-controller@ffffec00 {
				compatible = "atmel,at91sam9g45-dma";
				reg = <0xffffec00 0x200>;
				interrupts = <20 IRQ_TYPE_LEVEL_HIGH 0>;
				#dma-cells = <2>;
			};

			dma1: dma-controller@ffffee00 {
				compatible = "atmel,at91sam9g45-dma";
				reg = <0xffffee00 0x200>;
				interrupts = <21 IRQ_TYPE_LEVEL_HIGH 0>;
				#dma-cells = <2>;
			};

			pinctrl@fffff400 {
				#address-cells = <1>;
				#size-cells = <1>;
				compatible = "atmel,at91sam9x5-pinctrl", "atmel,at91rm9200-pinctrl", "simple-bus";
				ranges = <0xfffff400 0xfffff400 0x800>;

				/* shared pinctrl settings */
				dbgu {
					pinctrl_dbgu: dbgu-0 {
						atmel,pins =
							<AT91_PIOA 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA9 periph A */
							 AT91_PIOA 10 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA10 periph A with pullup */
					};
				};

				usart0 {
					pinctrl_usart0: usart0-0 {
						atmel,pins =
							<AT91_PIOA 0 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA0 periph A with pullup */
							 AT91_PIOA 1 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA1 periph A */
					};

					pinctrl_usart0_rts: usart0_rts-0 {
						atmel,pins =
							<AT91_PIOA 2 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA2 periph A */
					};

					pinctrl_usart0_cts: usart0_cts-0 {
						atmel,pins =
							<AT91_PIOA 3 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA3 periph A */
					};

					pinctrl_usart0_sck: usart0_sck-0 {
						atmel,pins =
							<AT91_PIOA 4 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA4 periph A */
					};
				};

				usart1 {
					pinctrl_usart1: usart1-0 {
						atmel,pins =
							<AT91_PIOA 5 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA5 periph A with pullup */
							 AT91_PIOA 6 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA6 periph A */
					};

					pinctrl_usart1_rts: usart1_rts-0 {
						atmel,pins =
							<AT91_PIOC 27 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC27 periph C */
					};

					pinctrl_usart1_cts: usart1_cts-0 {
						atmel,pins =
							<AT91_PIOC 28 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC28 periph C */
					};

					pinctrl_usart1_sck: usart1_sck-0 {
						atmel,pins =
							<AT91_PIOC 28 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC29 periph C */
					};
				};

				usart2 {
					pinctrl_usart2: usart2-0 {
						atmel,pins =
							<AT91_PIOA 7 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA7 periph A with pullup */
							 AT91_PIOA 8 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA8 periph A */
					};

					pinctrl_usart2_rts: usart2_rts-0 {
						atmel,pins =
							<AT91_PIOB 0 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB0 periph B */
					};

					pinctrl_usart2_cts: usart2_cts-0 {
						atmel,pins =
							<AT91_PIOB 1 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB1 periph B */
					};

					pinctrl_usart2_sck: usart2_sck-0 {
						atmel,pins =
							<AT91_PIOB 2 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB2 periph B */
					};
				};

				uart0 {
					pinctrl_uart0: uart0-0 {
						atmel,pins =
							<AT91_PIOC 8 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC8 periph C */
							 AT91_PIOC 9 AT91_PERIPH_C AT91_PINCTRL_PULL_UP>;	/* PC9 periph C with pullup */
					};
				};

				uart1 {
					pinctrl_uart1: uart1-0 {
						atmel,pins =
							<AT91_PIOC 16 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC16 periph C */
							 AT91_PIOC 17 AT91_PERIPH_C AT91_PINCTRL_PULL_UP>;	/* PC17 periph C with pullup */
					};
				};

				nand {
					pinctrl_nand: nand-0 {
						atmel,pins =
							<AT91_PIOD 0 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD0 periph A Read Enable */
							 AT91_PIOD 1 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD1 periph A Write Enable */
							 AT91_PIOD 2 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD2 periph A Address Latch Enable */
							 AT91_PIOD 3 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD3 periph A Command Latch Enable */
							 AT91_PIOD 4 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP	/* PD4 gpio Chip Enable pin pull_up */
							 AT91_PIOD 5 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP	/* PD5 gpio RDY/BUSY pin pull_up */
							 AT91_PIOD 6 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD6 periph A Data bit 0 */
							 AT91_PIOD 7 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD7 periph A Data bit 1 */
							 AT91_PIOD 8 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD8 periph A Data bit 2 */
							 AT91_PIOD 9 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD9 periph A Data bit 3 */
							 AT91_PIOD 10 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD10 periph A Data bit 4 */
							 AT91_PIOD 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD11 periph A Data bit 5 */
							 AT91_PIOD 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD12 periph A Data bit 6 */
							 AT91_PIOD 13 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD13 periph A Data bit 7 */
					};

					pinctrl_nand_16bits: nand_16bits-0 {
						atmel,pins =
							<AT91_PIOD 14 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD14 periph A Data bit 8 */
							 AT91_PIOD 15 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD15 periph A Data bit 9 */
							 AT91_PIOD 16 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD16 periph A Data bit 10 */
							 AT91_PIOD 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD17 periph A Data bit 11 */
							 AT91_PIOD 18 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD18 periph A Data bit 12 */
							 AT91_PIOD 19 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD19 periph A Data bit 13 */
							 AT91_PIOD 20 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PD20 periph A Data bit 14 */
							 AT91_PIOD 21 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PD21 periph A Data bit 15 */
					};
				};

				mmc0 {
					pinctrl_mmc0_slot0_clk_cmd_dat0: mmc0_slot0_clk_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 17 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA17 periph A */
							 AT91_PIOA 16 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA16 periph A with pullup */
							 AT91_PIOA 15 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA15 periph A with pullup */
					};

					pinctrl_mmc0_slot0_dat1_3: mmc0_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 18 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA18 periph A with pullup */
							 AT91_PIOA 19 AT91_PERIPH_A AT91_PINCTRL_PULL_UP	/* PA19 periph A with pullup */
							 AT91_PIOA 20 AT91_PERIPH_A AT91_PINCTRL_PULL_UP>;	/* PA20 periph A with pullup */
					};
				};

				mmc1 {
					pinctrl_mmc1_slot0_clk_cmd_dat0: mmc1_slot0_clk_cmd_dat0-0 {
						atmel,pins =
							<AT91_PIOA 13 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA13 periph B */
							 AT91_PIOA 12 AT91_PERIPH_B AT91_PINCTRL_PULL_UP	/* PA12 periph B with pullup */
							 AT91_PIOA 11 AT91_PERIPH_B AT91_PINCTRL_PULL_UP>;	/* PA11 periph B with pullup */
					};

					pinctrl_mmc1_slot0_dat1_3: mmc1_slot0_dat1_3-0 {
						atmel,pins =
							<AT91_PIOA 2 AT91_PERIPH_B AT91_PINCTRL_PULL_UP	/* PA2 periph B with pullup */
							 AT91_PIOA 3 AT91_PERIPH_B AT91_PINCTRL_PULL_UP	/* PA3 periph B with pullup */
							 AT91_PIOA 4 AT91_PERIPH_B AT91_PINCTRL_PULL_UP>;	/* PA4 periph B with pullup */
					};
				};

				ssc0 {
					pinctrl_ssc0_tx: ssc0_tx-0 {
						atmel,pins =
							<AT91_PIOA 24 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA24 periph B */
							 AT91_PIOA 25 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA25 periph B */
							 AT91_PIOA 26 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA26 periph B */
					};

					pinctrl_ssc0_rx: ssc0_rx-0 {
						atmel,pins =
							<AT91_PIOA 27 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA27 periph B */
							 AT91_PIOA 28 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA28 periph B */
							 AT91_PIOA 29 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA29 periph B */
					};
				};

				spi0 {
					pinctrl_spi0: spi0-0 {
						atmel,pins =
							<AT91_PIOA 11 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA11 periph A SPI0_MISO pin */
							 AT91_PIOA 12 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA12 periph A SPI0_MOSI pin */
							 AT91_PIOA 13 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA13 periph A SPI0_SPCK pin */
					};
				};

				spi1 {
					pinctrl_spi1: spi1-0 {
						atmel,pins =
							<AT91_PIOA 21 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA21 periph B SPI1_MISO pin */
							 AT91_PIOA 22 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PA22 periph B SPI1_MOSI pin */
							 AT91_PIOA 23 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PA23 periph B SPI1_SPCK pin */
					};
				};

				i2c0 {
					pinctrl_i2c0: i2c0-0 {
						atmel,pins =
							<AT91_PIOA 30 AT91_PERIPH_A AT91_PINCTRL_NONE	/* PA30 periph A I2C0 data */
							 AT91_PIOA 31 AT91_PERIPH_A AT91_PINCTRL_NONE>;	/* PA31 periph A I2C0 clock */
					};
				};

				i2c1 {
					pinctrl_i2c1: i2c1-0 {
						atmel,pins =
							<AT91_PIOC 0 AT91_PERIPH_C AT91_PINCTRL_NONE	/* PC0 periph C I2C1 data */
							 AT91_PIOC 1 AT91_PERIPH_C AT91_PINCTRL_NONE>;	/* PC1 periph C I2C1 clock */
					};
				};

				i2c2 {
					pinctrl_i2c2: i2c2-0 {
						atmel,pins =
							<AT91_PIOB 4 AT91_PERIPH_B AT91_PINCTRL_NONE	/* PB4 periph B I2C2 data */
							 AT91_PIOB 5 AT91_PERIPH_B AT91_PINCTRL_NONE>;	/* PB5 periph B I2C2 clock */
					};
				};

				i2c_gpio0 {
					pinctrl_i2c_gpio0: i2c_gpio0-0 {
						atmel,pins =
							<AT91_PIOA 30 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE	/* PA30 gpio multidrive I2C0 data */
							 AT91_PIOA 31 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE>;	/* PA31 gpio multidrive I2C0 clock */
					};
				};

				i2c_gpio1 {
					pinctrl_i2c_gpio1: i2c_gpio1-0 {
						atmel,pins =
							<AT91_PIOC 0 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE	/* PC0 gpio multidrive I2C1 data */
							 AT91_PIOC 1 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE>;	/* PC1 gpio multidrive I2C1 clock */
					};
				};

				i2c_gpio2 {
					pinctrl_i2c_gpio2: i2c_gpio2-0 {
						atmel,pins =
							<AT91_PIOB 4 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE	/* PB4 gpio multidrive I2C2 data */
							 AT91_PIOB 5 AT91_PERIPH_GPIO AT91_PINCTRL_MULTI_DRIVE>;	/* PB5 gpio multidrive I2C2 clock */
					};
				};

				tcb0 {
					pinctrl_tcb0_tclk0: tcb0_tclk0-0 {
						atmel,pins = <AT91_PIOA 24 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk1: tcb0_tclk1-0 {
						atmel,pins = <AT91_PIOA 25 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tclk2: tcb0_tclk2-0 {
						atmel,pins = <AT91_PIOA 26 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa0: tcb0_tioa0-0 {
						atmel,pins = <AT91_PIOA 21 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa1: tcb0_tioa1-0 {
						atmel,pins = <AT91_PIOA 22 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tioa2: tcb0_tioa2-0 {
						atmel,pins = <AT91_PIOA 23 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob0: tcb0_tiob0-0 {
						atmel,pins = <AT91_PIOA 27 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob1: tcb0_tiob1-0 {
						atmel,pins = <AT91_PIOA 28 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb0_tiob2: tcb0_tiob2-0 {
						atmel,pins = <AT91_PIOA 29 AT91_PERIPH_A AT91_PINCTRL_NONE>;
					};
				};

				tcb1 {
					pinctrl_tcb1_tclk0: tcb1_tclk0-0 {
						atmel,pins = <AT91_PIOC 4 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tclk1: tcb1_tclk1-0 {
						atmel,pins = <AT91_PIOC 7 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tclk2: tcb1_tclk2-0 {
						atmel,pins = <AT91_PIOC 14 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa0: tcb1_tioa0-0 {
						atmel,pins = <AT91_PIOC 2 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa1: tcb1_tioa1-0 {
						atmel,pins = <AT91_PIOC 5 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tioa2: tcb1_tioa2-0 {
						atmel,pins = <AT91_PIOC 12 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob0: tcb1_tiob0-0 {
						atmel,pins = <AT91_PIOC 3 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob1: tcb1_tiob1-0 {
						atmel,pins = <AT91_PIOC 6 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};

					pinctrl_tcb1_tiob2: tcb1_tiob2-0 {
						atmel,pins = <AT91_PIOC 13 AT91_PERIPH_C AT91_PINCTRL_NONE>;
					};
				};

				pioA: gpio@fffff400 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff400 0x200>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
				};

				pioB: gpio@fffff600 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff600 0x200>;
					interrupts = <2 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					#gpio-lines = <19>;
					interrupt-controller;
					#interrupt-cells = <2>;
				};

				pioC: gpio@fffff800 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffff800 0x200>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					interrupt-controller;
					#interrupt-cells = <2>;
				};

				pioD: gpio@fffffa00 {
					compatible = "atmel,at91sam9x5-gpio", "atmel,at91rm9200-gpio";
					reg = <0xfffffa00 0x200>;
					interrupts = <3 IRQ_TYPE_LEVEL_HIGH 1>;
					#gpio-cells = <2>;
					gpio-controller;
					#gpio-lines = <22>;
					interrupt-controller;
					#interrupt-cells = <2>;
				};
			};

			ssc0: ssc@f0010000 {
				compatible = "atmel,at91sam9g45-ssc";
				reg = <0xf0010000 0x4000>;
				interrupts = <28 IRQ_TYPE_LEVEL_HIGH 5>;
				dmas = <&dma0 1 AT91_DMA_CFG_PER_ID(13)>,
				       <&dma0 1 AT91_DMA_CFG_PER_ID(14)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_ssc0_tx &pinctrl_ssc0_rx>;
				status = "disabled";
			};

			mmc0: mmc@f0008000 {
				compatible = "atmel,hsmci";
				reg = <0xf0008000 0x600>;
				interrupts = <12 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma0 1 AT91_DMA_CFG_PER_ID(0)>;
				dma-names = "rxtx";
				pinctrl-names = "default";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};

			mmc1: mmc@f000c000 {
				compatible = "atmel,hsmci";
				reg = <0xf000c000 0x600>;
				interrupts = <26 IRQ_TYPE_LEVEL_HIGH 0>;
				dmas = <&dma1 1 AT91_DMA_CFG_PER_ID(0)>;
				dma-names = "rxtx";
				pinctrl-names = "default";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};

			dbgu: serial@fffff200 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xfffff200 0x200>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_dbgu>;
				status = "disabled";
			};

			usart0: serial@f801c000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf801c000 0x200>;
				interrupts = <5 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart0>;
				status = "disabled";
			};

			usart1: serial@f8020000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8020000 0x200>;
				interrupts = <6 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart1>;
				status = "disabled";
			};

			usart2: serial@f8024000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8024000 0x200>;
				interrupts = <7 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usart2>;
				status = "disabled";
			};

			i2c0: i2c@f8010000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf8010000 0x100>;
				interrupts = <9 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma0 1 AT91_DMA_CFG_PER_ID(7)>,
				       <&dma0 1 AT91_DMA_CFG_PER_ID(8)>;
				dma-names = "tx", "rx";
				#address-cells = <1>;
				#size-cells = <0>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c0>;
				status = "disabled";
			};

			i2c1: i2c@f8014000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf8014000 0x100>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma1 1 AT91_DMA_CFG_PER_ID(5)>,
				       <&dma1 1 AT91_DMA_CFG_PER_ID(6)>;
				dma-names = "tx", "rx";
				#address-cells = <1>;
				#size-cells = <0>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c1>;
				status = "disabled";
			};

			i2c2: i2c@f8018000 {
				compatible = "atmel,at91sam9x5-i2c";
				reg = <0xf8018000 0x100>;
				interrupts = <11 IRQ_TYPE_LEVEL_HIGH 6>;
				dmas = <&dma0 1 AT91_DMA_CFG_PER_ID(9)>,
				       <&dma0 1 AT91_DMA_CFG_PER_ID(10)>;
				dma-names = "tx", "rx";
				#address-cells = <1>;
				#size-cells = <0>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_i2c2>;
				status = "disabled";
			};

			uart0: serial@f8040000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8040000 0x200>;
				interrupts = <15 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_uart0>;
				status = "disabled";
			};

			uart1: serial@f8044000 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0xf8044000 0x200>;
				interrupts = <16 IRQ_TYPE_LEVEL_HIGH 5>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_uart1>;
				status = "disabled";
			};

			adc0: adc@f804c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91sam9260-adc";
				reg = <0xf804c000 0x100>;
				interrupts = <19 IRQ_TYPE_LEVEL_HIGH 0>;
				atmel,adc-use-external-triggers;
				atmel,adc-channels-used = <0xffff>;
				atmel,adc-vref = <3300>;
				atmel,adc-startup-time = <40>;
				atmel,adc-res = <8 10>;
				atmel,adc-res-names = "lowres", "highres";
				atmel,adc-use-res = "highres";

				trigger@0 {
					reg = <0>;
					trigger-name = "external-rising";
					trigger-value = <0x1>;
					trigger-external;
				};

				trigger@1 {
					reg = <1>;
					trigger-name = "external-falling";
					trigger-value = <0x2>;
					trigger-external;
				};

				trigger@2 {
					reg = <2>;
					trigger-name = "external-any";
					trigger-value = <0x3>;
					trigger-external;
				};

				trigger@3 {
					reg = <3>;
					trigger-name = "continuous";
					trigger-value = <0x6>;
				};
			};

			spi0: spi@f0000000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xf0000000 0x100>;
				interrupts = <13 IRQ_TYPE_LEVEL_HIGH 3>;
				dmas = <&dma0 1 AT91_DMA_CFG_PER_ID(1)>,
				       <&dma0 1 AT91_DMA_CFG_PER_ID(2)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi0>;
				status = "disabled";
			};

			spi1: spi@f0004000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91rm9200-spi";
				reg = <0xf0004000 0x100>;
				interrupts = <14 IRQ_TYPE_LEVEL_HIGH 3>;
				dmas = <&dma1 1 AT91_DMA_CFG_PER_ID(1)>,
				       <&dma1 1 AT91_DMA_CFG_PER_ID(2)>;
				dma-names = "tx", "rx";
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_spi1>;
				status = "disabled";
			};

			usb2: gadget@f803c000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "atmel,at91sam9rl-udc";
				reg = <0x00500000 0x80000
				       0xf803c000 0x400>;
				interrupts = <23 IRQ_TYPE_LEVEL_HIGH 0>;
				status = "disabled";

				ep0 {
					reg = <0>;
					atmel,fifo-size = <64>;
					atmel,nb-banks = <1>;
				};

				ep1 {
					reg = <1>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <2>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep2 {
					reg = <2>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <2>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep3 {
					reg = <3>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
				};

				ep4 {
					reg = <4>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
				};

				ep5 {
					reg = <5>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
					atmel,can-isoc;
				};

				ep6 {
					reg = <6>;
					atmel,fifo-size = <1024>;
					atmel,nb-banks = <3>;
					atmel,can-dma;
					atmel,can-isoc;
				};
			};

			watchdog@fffffe40 {
				compatible = "atmel,at91sam9260-wdt";
				reg = <0xfffffe40 0x10>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				atmel,watchdog-type = "hardware";
				atmel,reset-type = "all";
				atmel,dbg-halt;
				atmel,idle-halt;
				status = "disabled";
			};

			rtc@fffffeb0 {
				compatible = "atmel,at91sam9x5-rtc";
				reg = <0xfffffeb0 0x40>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH 7>;
				status = "disabled";
			};

			pwm0: pwm@f8034000 {
				compatible = "atmel,at91sam9rl-pwm";
				reg = <0xf8034000 0x300>;
				interrupts = <18 IRQ_TYPE_LEVEL_HIGH 4>;
				#pwm-cells = <3>;
				status = "disabled";
			};
		};

		nand0: nand@40000000 {
			compatible = "atmel,at91rm9200-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x40000000 0x10000000
			       0xffffe000 0x600		/* PMECC Registers */
			       0xffffe600 0x200		/* PMECC Error Location Registers */
			       0x00108000 0x18000	/* PMECC looup table in ROM code  */
			      >;
			atmel,pmecc-lookup-table-offset = <0x0 0x8000>;
			atmel,nand-addr-offset = <21>;
			atmel,nand-cmd-offset = <22>;
			atmel,nand-has-dma;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;
			gpios = <&pioD 5 GPIO_ACTIVE_HIGH
				 &pioD 4 GPIO_ACTIVE_HIGH
				 0
				>;
			status = "disabled";
		};

		usb0: ohci@00600000 {
			compatible = "atmel,at91rm9200-ohci", "usb-ohci";
			reg = <0x00600000 0x100000>;
			interrupts = <22 IRQ_TYPE_LEVEL_HIGH 2>;
			status = "disabled";
		};

		usb1: ehci@00700000 {
			compatible = "atmel,at91sam9g45-ehci", "usb-ehci";
			reg = <0x00700000 0x100000>;
			interrupts = <22 IRQ_TYPE_LEVEL_HIGH 2>;
			status = "disabled";
		};
	};

	i2c@0 {
		compatible = "i2c-gpio";
		gpios = <&pioA 30 GPIO_ACTIVE_HIGH /* sda */
			 &pioA 31 GPIO_ACTIVE_HIGH /* scl */
			>;
		i2c-gpio,sda-open-drain;
		i2c-gpio,scl-open-drain;
		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
		#address-cells = <1>;
		#size-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c_gpio0>;
		status = "disabled";
	};

	i2c@1 {
		compatible = "i2c-gpio";
		gpios = <&pioC 0 GPIO_ACTIVE_HIGH /* sda */
			 &pioC 1 GPIO_ACTIVE_HIGH /* scl */
			>;
		i2c-gpio,sda-open-drain;
		i2c-gpio,scl-open-drain;
		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
		#address-cells = <1>;
		#size-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c_gpio1>;
		status = "disabled";
	};

	i2c@2 {
		compatible = "i2c-gpio";
		gpios = <&pioB 4 GPIO_ACTIVE_HIGH /* sda */
			 &pioB 5 GPIO_ACTIVE_HIGH /* scl */
			>;
		i2c-gpio,sda-open-drain;
		i2c-gpio,scl-open-drain;
		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
		#address-cells = <1>;
		#size-cells = <0>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c_gpio2>;
		status = "disabled";
	};
};
