/*
 * Copyright 2013 Freescale Semiconductor, Inc.
 *
 * Author: Fabio Estevam <fabio.estevam@freescale.com>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 *
 */

/dts-v1/;
#include "imx6q.dtsi"

/ {
	model = "Udoo i.MX6 Quad Board";
	compatible = "udoo,imx6q-udoo", "fsl,imx6q";

	memory {
		reg = <0x10000000 0x40000000>;
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	status = "okay";
};

&iomuxc {
	imx6q-udoo {
		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
				MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
			>;
		};

		pinctrl_uart2: uart2grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D26__UART2_TX_DATA	0x1b0b1
				MX6QDL_PAD_EIM_D27__UART2_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_usdhc3: usdhc3grp {
			fsl,pins = <
				MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17059
				MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10059
				MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
				MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
				MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
				MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
			>;
		};
	};
};

&sata {
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	non-removable;
	status = "okay";
};
