/*
 * Suppport for CompuLab SBC-T3730 with CM-T3730
 */

#include "omap3-cm-t3730.dts"
#include "omap3-sb-t35.dtsi"

/ {
	model = "CompuLab SBC-T3730 with CM-T3730";
	compatible = "compulab,omap3-sbc-t3730", "compulab,omap3-cm-t3730", "ti,omap36xx", "ti,omap3";
};

&omap3_pmx_core {
	pinctrl-names = "default";
	pinctrl-0 = <&sb_t35_usb_hub_pins>;

	sb_t35_usb_hub_pins: pinmux_sb_t35_usb_hub_pins {
		pinctrl-single,pins = <
			OMAP3_CORE1_IOPAD(0x2130, PIN_OUTPUT | MUX_MODE4) /* ccdc_wen.gpio_167 - SB-T35 USB HUB RST */
		>;
	};
};

&gpmc {
	ranges = <5 0 0x2c000000 0x01000000>,
		 <4 0 0x2d000000 0x01000000>;
};
