/*
 * Copyright (C) 2012 Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
 *
 * This file is licensed under the terms of the GNU General Public
 * License version 2. This program is licensed "as is" without any
 * warranty of any kind, whether express or implied.
 */

/dts-v1/;
/include/ "orion5x.dtsi"

/ {
	model = "LaCie Ethernet Disk mini V2";
	compatible = "lacie,ethernet-disk-mini-v2", "marvell,orion5x-88f5182", "marvell,orion5x";

	memory {
		reg = <0x00000000 0x4000000>; /* 64 MB */
	};

	chosen {
		bootargs = "console=ttyS0,115200n8 earlyprintk";
	};

	ocp@f1000000 {
		serial@12000 {
			clock-frequency = <166666667>;
			status = "okay";
		};

		sata@80000 {
			status = "okay";
			nr-ports = <2>;
		};
	};

	gpio_keys {
		compatible = "gpio-keys";
		#address-cells = <1>;
		#size-cells = <0>;
		button@1 {
			label = "Power-on Switch";
			linux,code = <116>; /* KEY_POWER */
			gpios = <&gpio0 18 0>;
		};
	};

	gpio_leds {
		compatible = "gpio-leds";

		led@1 {
			label = "power:blue";
			gpios = <&gpio0 16 1>;
		};
	};
};

&mdio {
	status = "okay";

	ethphy: ethernet-phy {
		reg = <8>;
	};
};

&eth {
	status = "okay";

	ethernet-port@0 {
		phy-handle = <&ethphy>;
	};
};
