#include "skeleton.dtsi"

/ {
	soc {
		compatible = "simple-bus";
		model = "Ingenic JZ4755";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		serial0: serial@b0030000 {
			compatible = "ingenic,jz4740-uart";
			reg = <0xb0030000 0x20>;
			reg-shift = <2>;
			clock-frequency = <12000000>;
			status = "disabled";
		};

		serial1: serial@b0031000 {
			compatible = "ingenic,jz4740-uart";
			reg = <0xb0031000 0x20>;
			reg-shift = <2>;
			clock-frequency = <12000000>;
			status = "disabled";
		};

		serial2: serial@b0032000 {
			compatible = "ingenic,jz4740-uart";
			reg = <0xb0032000 0x20>;
			reg-shift = <2>;
			clock-frequency = <12000000>;
			status = "disabled";
		};
	};
};
