/*
 * Device Tree Source for DRA7xx clock data
 *
 * Copyright (C) 2013 Texas Instruments, Inc.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
&cm_core_aon_clocks {
	atl_clkin0_ck: atl_clkin0_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	atl_clkin1_ck: atl_clkin1_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	atl_clkin2_ck: atl_clkin2_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	atlclkin3_ck: atlclkin3_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	hdmi_clkin_ck: hdmi_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	mlb_clkin_ck: mlb_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	mlbp_clkin_ck: mlbp_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	pciesref_acs_clk_ck: pciesref_acs_clk_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <100000000>;
	};

	ref_clkin0_ck: ref_clkin0_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	ref_clkin1_ck: ref_clkin1_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	ref_clkin2_ck: ref_clkin2_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	ref_clkin3_ck: ref_clkin3_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	rmii_clk_ck: rmii_clk_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	sdvenc_clkin_ck: sdvenc_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	secure_32k_clk_src_ck: secure_32k_clk_src_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <32768>;
	};

	sys_32k_ck: sys_32k_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <32768>;
	};

	virt_12000000_ck: virt_12000000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <12000000>;
	};

	virt_13000000_ck: virt_13000000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <13000000>;
	};

	virt_16800000_ck: virt_16800000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <16800000>;
	};

	virt_19200000_ck: virt_19200000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <19200000>;
	};

	virt_20000000_ck: virt_20000000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <20000000>;
	};

	virt_26000000_ck: virt_26000000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <26000000>;
	};

	virt_27000000_ck: virt_27000000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <27000000>;
	};

	virt_38400000_ck: virt_38400000_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <38400000>;
	};

	sys_clkin2: sys_clkin2 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <22579200>;
	};

	usb_otg_clkin_ck: usb_otg_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	video1_clkin_ck: video1_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	video1_m2_clkin_ck: video1_m2_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	video2_clkin_ck: video2_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	video2_m2_clkin_ck: video2_m2_clkin_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};

	dpll_abe_ck: dpll_abe_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-m4xen-clock";
		clocks = <&abe_dpll_clk_mux>, <&abe_dpll_bypass_clk_mux>;
		reg = <0x01e0>, <0x01e4>, <0x01ec>, <0x01e8>;
	};

	dpll_abe_x2_ck: dpll_abe_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_abe_ck>;
	};

	dpll_abe_m2x2_ck: dpll_abe_m2x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_x2_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x01f0>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	abe_clk: abe_clk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_m2x2_ck>;
		ti,max-div = <4>;
		reg = <0x0108>;
		ti,index-power-of-two;
	};

	dpll_abe_m2_ck: dpll_abe_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x01f0>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_abe_m3x2_ck: dpll_abe_m3x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_x2_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x01f4>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_ck: dpll_core_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-core-clock";
		clocks = <&sys_clkin1>, <&dpll_abe_m3x2_ck>;
		reg = <0x0120>, <0x0124>, <0x012c>, <0x0128>;
	};

	dpll_core_x2_ck: dpll_core_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_core_ck>;
	};

	dpll_core_h12x2_ck: dpll_core_h12x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x013c>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	mpu_dpll_hs_clk_div: mpu_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_h12x2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_mpu_ck: dpll_mpu_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&mpu_dpll_hs_clk_div>;
		reg = <0x0160>, <0x0164>, <0x016c>, <0x0168>;
	};

	dpll_mpu_m2_ck: dpll_mpu_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_mpu_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0170>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	mpu_dclk_div: mpu_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_mpu_m2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dsp_dpll_hs_clk_div: dsp_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_h12x2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_dsp_ck: dpll_dsp_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&dsp_dpll_hs_clk_div>;
		reg = <0x0234>, <0x0238>, <0x0240>, <0x023c>;
	};

	dpll_dsp_m2_ck: dpll_dsp_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_dsp_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0244>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	iva_dpll_hs_clk_div: iva_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_h12x2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_iva_ck: dpll_iva_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&iva_dpll_hs_clk_div>;
		reg = <0x01a0>, <0x01a4>, <0x01ac>, <0x01a8>;
	};

	dpll_iva_m2_ck: dpll_iva_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_iva_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x01b0>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	iva_dclk: iva_dclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_iva_m2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_gpu_ck: dpll_gpu_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&dpll_abe_m3x2_ck>;
		reg = <0x02d8>, <0x02dc>, <0x02e4>, <0x02e0>;
	};

	dpll_gpu_m2_ck: dpll_gpu_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gpu_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x02e8>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_m2_ck: dpll_core_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0130>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	core_dpll_out_dclk_div: core_dpll_out_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_m2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_ddr_ck: dpll_ddr_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&dpll_abe_m3x2_ck>;
		reg = <0x0210>, <0x0214>, <0x021c>, <0x0218>;
	};

	dpll_ddr_m2_ck: dpll_ddr_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_ddr_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0220>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_gmac_ck: dpll_gmac_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&dpll_abe_m3x2_ck>;
		reg = <0x02a8>, <0x02ac>, <0x02b4>, <0x02b0>;
	};

	dpll_gmac_m2_ck: dpll_gmac_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x02b8>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	video2_dclk_div: video2_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video2_m2_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	video1_dclk_div: video1_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video1_m2_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	hdmi_dclk_div: hdmi_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&hdmi_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	per_dpll_hs_clk_div: per_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_abe_m3x2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	usb_dpll_hs_clk_div: usb_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_abe_m3x2_ck>;
		clock-mult = <1>;
		clock-div = <3>;
	};

	eve_dpll_hs_clk_div: eve_dpll_hs_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_h12x2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_eve_ck: dpll_eve_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&eve_dpll_hs_clk_div>;
		reg = <0x0284>, <0x0288>, <0x0290>, <0x028c>;
	};

	dpll_eve_m2_ck: dpll_eve_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_eve_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0294>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	eve_dclk_div: eve_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_eve_m2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_core_h13x2_ck: dpll_core_h13x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0140>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_h14x2_ck: dpll_core_h14x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0144>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_h22x2_ck: dpll_core_h22x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0154>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_h23x2_ck: dpll_core_h23x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0158>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_core_h24x2_ck: dpll_core_h24x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_core_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x015c>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_ddr_x2_ck: dpll_ddr_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_ddr_ck>;
	};

	dpll_ddr_h11x2_ck: dpll_ddr_h11x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_ddr_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0228>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_dsp_x2_ck: dpll_dsp_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_dsp_ck>;
	};

	dpll_dsp_m3x2_ck: dpll_dsp_m3x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_dsp_x2_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0248>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_gmac_x2_ck: dpll_gmac_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_gmac_ck>;
	};

	dpll_gmac_h11x2_ck: dpll_gmac_h11x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x02c0>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_gmac_h12x2_ck: dpll_gmac_h12x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x02c4>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_gmac_h13x2_ck: dpll_gmac_h13x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x02c8>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_gmac_m3x2_ck: dpll_gmac_m3x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_x2_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x02bc>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	gmii_m_clk_div: gmii_m_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_gmac_h11x2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	hdmi_clk2_div: hdmi_clk2_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&hdmi_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	hdmi_div_clk: hdmi_div_clk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&hdmi_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	l3_iclk_div: l3_iclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_core_h12x2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	l4_root_clk_div: l4_root_clk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&l3_iclk_div>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	video1_clk2_div: video1_clk2_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video1_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	video1_div_clk: video1_div_clk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video1_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	video2_clk2_div: video2_clk2_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video2_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	video2_div_clk: video2_div_clk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&video2_clkin_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	ipu1_gfclk_mux: ipu1_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&dpll_abe_m2x2_ck>, <&dpll_core_h22x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x0520>;
	};

	mcasp1_ahclkr_mux: mcasp1_ahclkr_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <28>;
		reg = <0x0550>;
	};

	mcasp1_ahclkx_mux: mcasp1_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x0550>;
	};

	mcasp1_aux_gfclk_mux: mcasp1_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x0550>;
	};

	timer5_gfclk_mux: timer5_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>, <&clkoutmux0_clk_mux>;
		ti,bit-shift = <24>;
		reg = <0x0558>;
	};

	timer6_gfclk_mux: timer6_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>, <&clkoutmux0_clk_mux>;
		ti,bit-shift = <24>;
		reg = <0x0560>;
	};

	timer7_gfclk_mux: timer7_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>, <&clkoutmux0_clk_mux>;
		ti,bit-shift = <24>;
		reg = <0x0568>;
	};

	timer8_gfclk_mux: timer8_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>, <&clkoutmux0_clk_mux>;
		ti,bit-shift = <24>;
		reg = <0x0570>;
	};

	uart6_gfclk_mux: uart6_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x0580>;
	};

	dummy_ck: dummy_ck {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <0>;
	};
};
&prm_clocks {
	sys_clkin1: sys_clkin1 {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&virt_12000000_ck>, <&virt_20000000_ck>, <&virt_16800000_ck>, <&virt_19200000_ck>, <&virt_26000000_ck>, <&virt_27000000_ck>, <&virt_38400000_ck>;
		reg = <0x0110>;
		ti,index-starts-at-one;
	};

	abe_dpll_sys_clk_mux: abe_dpll_sys_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>;
		reg = <0x0118>;
	};

	abe_dpll_bypass_clk_mux: abe_dpll_bypass_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_dpll_sys_clk_mux>, <&sys_32k_ck>;
		reg = <0x0114>;
	};

	abe_dpll_clk_mux: abe_dpll_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_dpll_sys_clk_mux>, <&sys_32k_ck>;
		reg = <0x010c>;
	};

	abe_24m_fclk: abe_24m_fclk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_m2x2_ck>;
		reg = <0x011c>;
		ti,dividers = <8>, <16>;
	};

	aess_fclk: aess_fclk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&abe_clk>;
		reg = <0x0178>;
		ti,max-div = <2>;
	};

	abe_giclk_div: abe_giclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&aess_fclk>;
		reg = <0x0174>;
		ti,max-div = <2>;
	};

	abe_lp_clk_div: abe_lp_clk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_m2x2_ck>;
		reg = <0x01d8>;
		ti,dividers = <16>, <32>;
	};

	abe_sys_clk_div: abe_sys_clk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin1>;
		reg = <0x0120>;
		ti,max-div = <2>;
	};

	adc_gfclk_mux: adc_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>, <&sys_32k_ck>;
		reg = <0x01dc>;
	};

	sys_clk1_dclk_div: sys_clk1_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin1>;
		ti,max-div = <64>;
		reg = <0x01c8>;
		ti,index-power-of-two;
	};

	sys_clk2_dclk_div: sys_clk2_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin2>;
		ti,max-div = <64>;
		reg = <0x01cc>;
		ti,index-power-of-two;
	};

	per_abe_x1_dclk_div: per_abe_x1_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_m2_ck>;
		ti,max-div = <64>;
		reg = <0x01bc>;
		ti,index-power-of-two;
	};

	dsp_gclk_div: dsp_gclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_dsp_m2_ck>;
		ti,max-div = <64>;
		reg = <0x018c>;
		ti,index-power-of-two;
	};

	gpu_dclk: gpu_dclk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gpu_m2_ck>;
		ti,max-div = <64>;
		reg = <0x01a0>;
		ti,index-power-of-two;
	};

	emif_phy_dclk_div: emif_phy_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_ddr_m2_ck>;
		ti,max-div = <64>;
		reg = <0x0190>;
		ti,index-power-of-two;
	};

	gmac_250m_dclk_div: gmac_250m_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_m2_ck>;
		ti,max-div = <64>;
		reg = <0x019c>;
		ti,index-power-of-two;
	};

	l3init_480m_dclk_div: l3init_480m_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_usb_m2_ck>;
		ti,max-div = <64>;
		reg = <0x01ac>;
		ti,index-power-of-two;
	};

	usb_otg_dclk_div: usb_otg_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&usb_otg_clkin_ck>;
		ti,max-div = <64>;
		reg = <0x0184>;
		ti,index-power-of-two;
	};

	sata_dclk_div: sata_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin1>;
		ti,max-div = <64>;
		reg = <0x01c0>;
		ti,index-power-of-two;
	};

	pcie2_dclk_div: pcie2_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_pcie_ref_m2_ck>;
		ti,max-div = <64>;
		reg = <0x01b8>;
		ti,index-power-of-two;
	};

	pcie_dclk_div: pcie_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&apll_pcie_m2_ck>;
		ti,max-div = <64>;
		reg = <0x01b4>;
		ti,index-power-of-two;
	};

	emu_dclk_div: emu_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin1>;
		ti,max-div = <64>;
		reg = <0x0194>;
		ti,index-power-of-two;
	};

	secure_32k_dclk_div: secure_32k_dclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&secure_32k_clk_src_ck>;
		ti,max-div = <64>;
		reg = <0x01c4>;
		ti,index-power-of-two;
	};

	clkoutmux0_clk_mux: clkoutmux0_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clk1_dclk_div>, <&sys_clk2_dclk_div>, <&per_abe_x1_dclk_div>, <&mpu_dclk_div>, <&dsp_gclk_div>, <&iva_dclk>, <&gpu_dclk>, <&core_dpll_out_dclk_div>, <&emif_phy_dclk_div>, <&gmac_250m_dclk_div>, <&video2_dclk_div>, <&video1_dclk_div>, <&hdmi_dclk_div>, <&func_96m_aon_dclk_div>, <&l3init_480m_dclk_div>, <&usb_otg_dclk_div>, <&sata_dclk_div>, <&pcie2_dclk_div>, <&pcie_dclk_div>, <&emu_dclk_div>, <&secure_32k_dclk_div>, <&eve_dclk_div>;
		reg = <0x0158>;
	};

	clkoutmux1_clk_mux: clkoutmux1_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clk1_dclk_div>, <&sys_clk2_dclk_div>, <&per_abe_x1_dclk_div>, <&mpu_dclk_div>, <&dsp_gclk_div>, <&iva_dclk>, <&gpu_dclk>, <&core_dpll_out_dclk_div>, <&emif_phy_dclk_div>, <&gmac_250m_dclk_div>, <&video2_dclk_div>, <&video1_dclk_div>, <&hdmi_dclk_div>, <&func_96m_aon_dclk_div>, <&l3init_480m_dclk_div>, <&usb_otg_dclk_div>, <&sata_dclk_div>, <&pcie2_dclk_div>, <&pcie_dclk_div>, <&emu_dclk_div>, <&secure_32k_dclk_div>, <&eve_dclk_div>;
		reg = <0x015c>;
	};

	clkoutmux2_clk_mux: clkoutmux2_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clk1_dclk_div>, <&sys_clk2_dclk_div>, <&per_abe_x1_dclk_div>, <&mpu_dclk_div>, <&dsp_gclk_div>, <&iva_dclk>, <&gpu_dclk>, <&core_dpll_out_dclk_div>, <&emif_phy_dclk_div>, <&gmac_250m_dclk_div>, <&video2_dclk_div>, <&video1_dclk_div>, <&hdmi_dclk_div>, <&func_96m_aon_dclk_div>, <&l3init_480m_dclk_div>, <&usb_otg_dclk_div>, <&sata_dclk_div>, <&pcie2_dclk_div>, <&pcie_dclk_div>, <&emu_dclk_div>, <&secure_32k_dclk_div>, <&eve_dclk_div>;
		reg = <0x0160>;
	};

	custefuse_sys_gfclk_div: custefuse_sys_gfclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&sys_clkin1>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	eve_clk: eve_clk {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&dpll_eve_m2_ck>, <&dpll_dsp_m3x2_ck>;
		reg = <0x0180>;
	};

	hdmi_dpll_clk_mux: hdmi_dpll_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>;
		reg = <0x01a4>;
	};

	mlb_clk: mlb_clk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mlb_clkin_ck>;
		ti,max-div = <64>;
		reg = <0x0134>;
		ti,index-power-of-two;
	};

	mlbp_clk: mlbp_clk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mlbp_clkin_ck>;
		ti,max-div = <64>;
		reg = <0x0130>;
		ti,index-power-of-two;
	};

	per_abe_x1_gfclk2_div: per_abe_x1_gfclk2_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_abe_m2_ck>;
		ti,max-div = <64>;
		reg = <0x0138>;
		ti,index-power-of-two;
	};

	timer_sys_clk_div: timer_sys_clk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&sys_clkin1>;
		reg = <0x0144>;
		ti,max-div = <2>;
	};

	video1_dpll_clk_mux: video1_dpll_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>;
		reg = <0x01d0>;
	};

	video2_dpll_clk_mux: video2_dpll_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>;
		reg = <0x01d4>;
	};

	wkupaon_iclk_mux: wkupaon_iclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&abe_lp_clk_div>;
		reg = <0x0108>;
	};

	gpio1_dbclk: gpio1_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1838>;
	};

	dcan1_sys_clk_mux: dcan1_sys_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_clkin1>, <&sys_clkin2>;
		ti,bit-shift = <24>;
		reg = <0x1888>;
	};

	timer1_gfclk_mux: timer1_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1840>;
	};

	uart10_gfclk_mux: uart10_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1880>;
	};
};
&cm_core_clocks {
	dpll_pcie_ref_ck: dpll_pcie_ref_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&sys_clkin1>;
		reg = <0x0200>, <0x0204>, <0x020c>, <0x0208>;
	};

	dpll_pcie_ref_m2ldo_ck: dpll_pcie_ref_m2ldo_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_pcie_ref_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0210>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	apll_pcie_in_clk_mux: apll_pcie_in_clk_mux@4ae06118 {
		compatible = "ti,mux-clock";
		clocks = <&dpll_pcie_ref_ck>, <&pciesref_acs_clk_ck>;
		#clock-cells = <0>;
		reg = <0x021c 0x4>;
		ti,bit-shift = <7>;
	};

	apll_pcie_ck: apll_pcie_ck {
		#clock-cells = <0>;
		compatible = "ti,dra7-apll-clock";
		clocks = <&apll_pcie_in_clk_mux>, <&dpll_pcie_ref_ck>;
		reg = <0x021c>, <0x0220>;
	};

	optfclk_pciephy_div: optfclk_pciephy_div@4a00821c {
		compatible = "ti,divider-clock";
		clocks = <&apll_pcie_ck>;
		#clock-cells = <0>;
		reg = <0x021c>;
		ti,bit-shift = <8>;
		ti,max-div = <2>;
	};

	optfclk_pciephy_clk: optfclk_pciephy_clk@4a0093b0 {
		compatible = "ti,gate-clock";
		clocks = <&apll_pcie_ck>;
		#clock-cells = <0>;
		reg = <0x13b0>;
		ti,bit-shift = <9>;
	};

	optfclk_pciephy_div_clk: optfclk_pciephy_div_clk@4a0093b0 {
		compatible = "ti,gate-clock";
		clocks = <&optfclk_pciephy_div>;
		#clock-cells = <0>;
		reg = <0x13b0>;
		ti,bit-shift = <10>;
	};

	apll_pcie_clkvcoldo: apll_pcie_clkvcoldo {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&apll_pcie_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	apll_pcie_clkvcoldo_div: apll_pcie_clkvcoldo_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&apll_pcie_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	apll_pcie_m2_ck: apll_pcie_m2_ck {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&apll_pcie_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_per_ck: dpll_per_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-clock";
		clocks = <&sys_clkin1>, <&per_dpll_hs_clk_div>;
		reg = <0x0140>, <0x0144>, <0x014c>, <0x0148>;
	};

	dpll_per_m2_ck: dpll_per_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0150>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	func_96m_aon_dclk_div: func_96m_aon_dclk_div {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	dpll_usb_ck: dpll_usb_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-j-type-clock";
		clocks = <&sys_clkin1>, <&usb_dpll_hs_clk_div>;
		reg = <0x0180>, <0x0184>, <0x018c>, <0x0188>;
	};

	dpll_usb_m2_ck: dpll_usb_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_usb_ck>;
		ti,max-div = <127>;
		ti,autoidle-shift = <8>;
		reg = <0x0190>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_pcie_ref_m2_ck: dpll_pcie_ref_m2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_pcie_ref_ck>;
		ti,max-div = <127>;
		ti,autoidle-shift = <8>;
		reg = <0x0210>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_per_x2_ck: dpll_per_x2_ck {
		#clock-cells = <0>;
		compatible = "ti,omap4-dpll-x2-clock";
		clocks = <&dpll_per_ck>;
	};

	dpll_per_h11x2_ck: dpll_per_h11x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0158>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_per_h12x2_ck: dpll_per_h12x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x015c>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_per_h13x2_ck: dpll_per_h13x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0160>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_per_h14x2_ck: dpll_per_h14x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_x2_ck>;
		ti,max-div = <63>;
		ti,autoidle-shift = <8>;
		reg = <0x0164>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_per_m2x2_ck: dpll_per_m2x2_ck {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_per_x2_ck>;
		ti,max-div = <31>;
		ti,autoidle-shift = <8>;
		reg = <0x0150>;
		ti,index-starts-at-one;
		ti,invert-autoidle-bit;
	};

	dpll_usb_clkdcoldo: dpll_usb_clkdcoldo {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_usb_ck>;
		clock-mult = <1>;
		clock-div = <1>;
	};

	func_128m_clk: func_128m_clk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_h11x2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	func_12m_fclk: func_12m_fclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_m2x2_ck>;
		clock-mult = <1>;
		clock-div = <16>;
	};

	func_24m_clk: func_24m_clk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_m2_ck>;
		clock-mult = <1>;
		clock-div = <4>;
	};

	func_48m_fclk: func_48m_fclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_m2x2_ck>;
		clock-mult = <1>;
		clock-div = <4>;
	};

	func_96m_fclk: func_96m_fclk {
		#clock-cells = <0>;
		compatible = "fixed-factor-clock";
		clocks = <&dpll_per_m2x2_ck>;
		clock-mult = <1>;
		clock-div = <2>;
	};

	l3init_60m_fclk: l3init_60m_fclk {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_usb_m2_ck>;
		reg = <0x0104>;
		ti,dividers = <1>, <8>;
	};

	dss_32khz_clk: dss_32khz_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <11>;
		reg = <0x1120>;
	};

	dss_48mhz_clk: dss_48mhz_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&func_48m_fclk>;
		ti,bit-shift = <9>;
		reg = <0x1120>;
	};

	dss_dss_clk: dss_dss_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&dpll_per_h12x2_ck>;
		ti,bit-shift = <8>;
		reg = <0x1120>;
	};

	dss_hdmi_clk: dss_hdmi_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&hdmi_dpll_clk_mux>;
		ti,bit-shift = <10>;
		reg = <0x1120>;
	};

	dss_video1_clk: dss_video1_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&video1_dpll_clk_mux>;
		ti,bit-shift = <12>;
		reg = <0x1120>;
	};

	dss_video2_clk: dss_video2_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&video2_dpll_clk_mux>;
		ti,bit-shift = <13>;
		reg = <0x1120>;
	};

	gpio2_dbclk: gpio2_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1760>;
	};

	gpio3_dbclk: gpio3_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1768>;
	};

	gpio4_dbclk: gpio4_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1770>;
	};

	gpio5_dbclk: gpio5_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1778>;
	};

	gpio6_dbclk: gpio6_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1780>;
	};

	gpio7_dbclk: gpio7_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1810>;
	};

	gpio8_dbclk: gpio8_dbclk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1818>;
	};

	mmc1_clk32k: mmc1_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1328>;
	};

	mmc2_clk32k: mmc2_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1330>;
	};

	mmc3_clk32k: mmc3_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1820>;
	};

	mmc4_clk32k: mmc4_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x1828>;
	};

	sata_ref_clk: sata_ref_clk {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_clkin1>;
		ti,bit-shift = <8>;
		reg = <0x1388>;
	};

	usb_otg_ss1_refclk960m: usb_otg_ss1_refclk960m {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&dpll_usb_clkdcoldo>;
		ti,bit-shift = <8>;
		reg = <0x13f0>;
	};

	usb_otg_ss2_refclk960m: usb_otg_ss2_refclk960m {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&dpll_usb_clkdcoldo>;
		ti,bit-shift = <8>;
		reg = <0x1340>;
	};

	usb_phy1_always_on_clk32k: usb_phy1_always_on_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x0640>;
	};

	usb_phy2_always_on_clk32k: usb_phy2_always_on_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x0688>;
	};

	usb_phy3_always_on_clk32k: usb_phy3_always_on_clk32k {
		#clock-cells = <0>;
		compatible = "ti,gate-clock";
		clocks = <&sys_32k_ck>;
		ti,bit-shift = <8>;
		reg = <0x0698>;
	};

	atl_dpll_clk_mux: atl_dpll_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&sys_32k_ck>, <&video1_clkin_ck>, <&video2_clkin_ck>, <&hdmi_clkin_ck>;
		ti,bit-shift = <24>;
		reg = <0x0c00>;
	};

	atl_gfclk_mux: atl_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&l3_iclk_div>, <&dpll_abe_m2_ck>, <&atl_dpll_clk_mux>;
		ti,bit-shift = <26>;
		reg = <0x0c00>;
	};

	gmac_gmii_ref_clk_div: gmac_gmii_ref_clk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&dpll_gmac_m2_ck>;
		ti,bit-shift = <24>;
		reg = <0x13d0>;
		ti,dividers = <2>;
	};

	gmac_rft_clk_mux: gmac_rft_clk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&video1_clkin_ck>, <&video2_clkin_ck>, <&dpll_abe_m2_ck>, <&hdmi_clkin_ck>, <&l3_iclk_div>;
		ti,bit-shift = <25>;
		reg = <0x13d0>;
	};

	gpu_core_gclk_mux: gpu_core_gclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&dpll_core_h14x2_ck>, <&dpll_per_h14x2_ck>, <&dpll_gpu_m2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1220>;
	};

	gpu_hyd_gclk_mux: gpu_hyd_gclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&dpll_core_h14x2_ck>, <&dpll_per_h14x2_ck>, <&dpll_gpu_m2_ck>;
		ti,bit-shift = <26>;
		reg = <0x1220>;
	};

	l3instr_ts_gclk_div: l3instr_ts_gclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&wkupaon_iclk_mux>;
		ti,bit-shift = <24>;
		reg = <0x0e50>;
		ti,dividers = <8>, <16>, <32>;
	};

	mcasp2_ahclkr_mux: mcasp2_ahclkr_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <28>;
		reg = <0x1860>;
	};

	mcasp2_ahclkx_mux: mcasp2_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1860>;
	};

	mcasp2_aux_gfclk_mux: mcasp2_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1860>;
	};

	mcasp3_ahclkx_mux: mcasp3_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1868>;
	};

	mcasp3_aux_gfclk_mux: mcasp3_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1868>;
	};

	mcasp4_ahclkx_mux: mcasp4_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1898>;
	};

	mcasp4_aux_gfclk_mux: mcasp4_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1898>;
	};

	mcasp5_ahclkx_mux: mcasp5_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1878>;
	};

	mcasp5_aux_gfclk_mux: mcasp5_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1878>;
	};

	mcasp6_ahclkx_mux: mcasp6_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1904>;
	};

	mcasp6_aux_gfclk_mux: mcasp6_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1904>;
	};

	mcasp7_ahclkx_mux: mcasp7_ahclkx_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <24>;
		reg = <0x1908>;
	};

	mcasp7_aux_gfclk_mux: mcasp7_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <22>;
		reg = <0x1908>;
	};

	mcasp8_ahclk_mux: mcasp8_ahclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&abe_24m_fclk>, <&abe_sys_clk_div>, <&func_24m_clk>, <&atlclkin3_ck>, <&atl_clkin2_ck>, <&atl_clkin1_ck>, <&atl_clkin0_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&mlb_clk>, <&mlbp_clk>;
		ti,bit-shift = <22>;
		reg = <0x1890>;
	};

	mcasp8_aux_gfclk_mux: mcasp8_aux_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&per_abe_x1_gfclk2_div>, <&video1_clk2_div>, <&video2_clk2_div>, <&hdmi_clk2_div>;
		ti,bit-shift = <24>;
		reg = <0x1890>;
	};

	mmc1_fclk_mux: mmc1_fclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_128m_clk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1328>;
	};

	mmc1_fclk_div: mmc1_fclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mmc1_fclk_mux>;
		ti,bit-shift = <25>;
		ti,max-div = <4>;
		reg = <0x1328>;
		ti,index-power-of-two;
	};

	mmc2_fclk_mux: mmc2_fclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_128m_clk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1330>;
	};

	mmc2_fclk_div: mmc2_fclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mmc2_fclk_mux>;
		ti,bit-shift = <25>;
		ti,max-div = <4>;
		reg = <0x1330>;
		ti,index-power-of-two;
	};

	mmc3_gfclk_mux: mmc3_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1820>;
	};

	mmc3_gfclk_div: mmc3_gfclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mmc3_gfclk_mux>;
		ti,bit-shift = <25>;
		ti,max-div = <4>;
		reg = <0x1820>;
		ti,index-power-of-two;
	};

	mmc4_gfclk_mux: mmc4_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1828>;
	};

	mmc4_gfclk_div: mmc4_gfclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&mmc4_gfclk_mux>;
		ti,bit-shift = <25>;
		ti,max-div = <4>;
		reg = <0x1828>;
		ti,index-power-of-two;
	};

	qspi_gfclk_mux: qspi_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_128m_clk>, <&dpll_per_h13x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1838>;
	};

	qspi_gfclk_div: qspi_gfclk_div {
		#clock-cells = <0>;
		compatible = "ti,divider-clock";
		clocks = <&qspi_gfclk_mux>;
		ti,bit-shift = <25>;
		ti,max-div = <4>;
		reg = <0x1838>;
		ti,index-power-of-two;
	};

	timer10_gfclk_mux: timer10_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1728>;
	};

	timer11_gfclk_mux: timer11_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1730>;
	};

	timer13_gfclk_mux: timer13_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x17c8>;
	};

	timer14_gfclk_mux: timer14_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x17d0>;
	};

	timer15_gfclk_mux: timer15_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x17d8>;
	};

	timer16_gfclk_mux: timer16_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1830>;
	};

	timer2_gfclk_mux: timer2_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1738>;
	};

	timer3_gfclk_mux: timer3_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1740>;
	};

	timer4_gfclk_mux: timer4_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1748>;
	};

	timer9_gfclk_mux: timer9_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&timer_sys_clk_div>, <&sys_32k_ck>, <&sys_clkin2>, <&ref_clkin0_ck>, <&ref_clkin1_ck>, <&ref_clkin2_ck>, <&ref_clkin3_ck>, <&abe_giclk_div>, <&video1_div_clk>, <&video2_div_clk>, <&hdmi_div_clk>;
		ti,bit-shift = <24>;
		reg = <0x1750>;
	};

	uart1_gfclk_mux: uart1_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1840>;
	};

	uart2_gfclk_mux: uart2_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1848>;
	};

	uart3_gfclk_mux: uart3_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1850>;
	};

	uart4_gfclk_mux: uart4_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1858>;
	};

	uart5_gfclk_mux: uart5_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1870>;
	};

	uart7_gfclk_mux: uart7_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x18d0>;
	};

	uart8_gfclk_mux: uart8_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x18e0>;
	};

	uart9_gfclk_mux: uart9_gfclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&func_48m_fclk>, <&dpll_per_m2x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x18e8>;
	};

	vip1_gclk_mux: vip1_gclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&l3_iclk_div>, <&dpll_core_h23x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1020>;
	};

	vip2_gclk_mux: vip2_gclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&l3_iclk_div>, <&dpll_core_h23x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1028>;
	};

	vip3_gclk_mux: vip3_gclk_mux {
		#clock-cells = <0>;
		compatible = "ti,mux-clock";
		clocks = <&l3_iclk_div>, <&dpll_core_h23x2_ck>;
		ti,bit-shift = <24>;
		reg = <0x1030>;
	};
};

&cm_core_clockdomains {
	coreaon_clkdm: coreaon_clkdm {
		compatible = "ti,clockdomain";
		clocks = <&dpll_usb_ck>;
	};
};
