/*
 * Copyright (C) 2011 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/*
 * Integrated Power Management Chip
 * http://www.ti.com/lit/ds/symlink/twl6030.pdf
 */
&twl {
	compatible = "ti,twl6030";
	interrupt-controller;
	#interrupt-cells = <1>;

	rtc {
		compatible = "ti,twl4030-rtc";
		interrupts = <11>;
	};

	vaux1: regulator-vaux1 {
		compatible = "ti,twl6030-vaux1";
		regulator-min-microvolt = <1000000>;
		regulator-max-microvolt = <3000000>;
	};

	vaux2: regulator-vaux2 {
		compatible = "ti,twl6030-vaux2";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <2800000>;
	};

	vaux3: regulator-vaux3 {
		compatible = "ti,twl6030-vaux3";
		regulator-min-microvolt = <1000000>;
		regulator-max-microvolt = <3000000>;
	};

	vmmc: regulator-vmmc {
		compatible = "ti,twl6030-vmmc";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <3000000>;
	};

	vpp: regulator-vpp {
		compatible = "ti,twl6030-vpp";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <2500000>;
	};

	vusim: regulator-vusim {
		compatible = "ti,twl6030-vusim";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <2900000>;
	};

	vdac: regulator-vdac {
		compatible = "ti,twl6030-vdac";
	};

	vana: regulator-vana {
		compatible = "ti,twl6030-vana";
	};

	vcxio: regulator-vcxio {
		compatible = "ti,twl6030-vcxio";
		regulator-always-on;
	};

	vusb: regulator-vusb {
		compatible = "ti,twl6030-vusb";
	};

	v1v8: regulator-v1v8 {
		compatible = "ti,twl6030-v1v8";
		regulator-always-on;
	};

	v2v1: regulator-v2v1 {
		compatible = "ti,twl6030-v2v1";
		regulator-always-on;
	};

	clk32kg: regulator-clk32kg {
		compatible = "ti,twl6030-clk32kg";
	};

	twl_usb_comparator: usb-comparator {
		compatible = "ti,twl6030-usb";
		interrupts = <4>, <10>;
	};

	twl_pwm: pwm {
		/* provides two PWMs (id 0, 1 for PWM1 and PWM2) */
		compatible = "ti,twl6030-pwm";
		#pwm-cells = <2>;
	};

	twl_pwmled: pwmled {
		/* provides one PWM (id 0 for Charging indicator LED) */
		compatible = "ti,twl6030-pwmled";
		#pwm-cells = <2>;
	};
};
