#include <dt-bindings/clock/ar933x-clk.h>

#include "skeleton.dtsi"

/ {
	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		device_type = "soc";
		ranges;

		serial0: serial@b8020000 {
			compatible = "qca,ar9330-uart";
			reg = <0xb8020000 0x14>;
			clocks = <&ar9331_clk AR933X_CLK_UART>;
			status = "disabled";
		};

		ar9331_clk: clock {
			compatible = "qca,ar933x-clk";
			reg = <0xb8050000 0x48>;
			#clock-cells = <1>;
		};

		spi: spi@bf000000{
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "qca,ath79-spi";
			reg = <0xbf000000 0x01000000>;
			status = "disabled";
		};
	};
};
