/*
 * Copyright 2013-2014 Texas Instruments, Inc.
 *
 * Keystone 2 Kepler/Hawking EVM device tree
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "keystone.dtsi"
#include "k2hk.dtsi"

/ {
	compatible =  "ti,k2hk-evm","ti,keystone";
	model = "Texas Instruments Keystone 2 Kepler/Hawking EVM";

	soc {
		clocks {
			refclksys: refclksys {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <122880000>;
				clock-output-names = "refclk-sys";
			};

			refclkpass: refclkpass {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <122880000>;
				clock-output-names = "refclk-pass";
			};

			refclkarm: refclkarm {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <125000000>;
				clock-output-names = "refclk-arm";
			};

			refclkddr3a: refclkddr3a {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <100000000>;
				clock-output-names = "refclk-ddr3a";
			};

			refclkddr3b: refclkddr3b {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <100000000>;
				clock-output-names = "refclk-ddr3b";
			};
		};
	};

	leds {
		compatible = "gpio-leds";
		debug1_1 {
			label = "keystone:green:debug1";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>; /* 12 */
		};

		debug1_2 {
			label = "keystone:red:debug1";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>; /* 13 */
		};

		debug2 {
			label = "keystone:blue:debug2";
			gpios = <&gpio0 14 GPIO_ACTIVE_HIGH>; /* 14 */
		};

		debug3 {
			label = "keystone:blue:debug3";
			gpios = <&gpio0 15 GPIO_ACTIVE_HIGH>; /* 15 */
		};
	};
};

&usb_phy {
	status = "okay";
};

&usb {
	status = "okay";
};

&aemif {
	cs0 {
		#address-cells = <2>;
		#size-cells = <1>;
		clock-ranges;
		ranges;

		ti,cs-chipselect = <0>;
		/* all timings in nanoseconds */
		ti,cs-min-turnaround-ns = <12>;
		ti,cs-read-hold-ns = <6>;
		ti,cs-read-strobe-ns = <23>;
		ti,cs-read-setup-ns = <9>;
		ti,cs-write-hold-ns = <8>;
		ti,cs-write-strobe-ns = <23>;
		ti,cs-write-setup-ns = <8>;

		nand@0,0 {
			compatible = "ti,keystone-nand","ti,davinci-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0 0 0x4000000
			       1 0 0x0000100>;

			ti,davinci-chipselect = <0>;
			ti,davinci-mask-ale = <0x2000>;
			ti,davinci-mask-cle = <0x4000>;
			ti,davinci-mask-chipsel = <0>;
			nand-ecc-mode = "hw";
			ti,davinci-ecc-bits = <4>;
			nand-on-flash-bbt;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x100000>;
				read-only;
			};

			partition@100000 {
				label = "params";
				reg = <0x100000 0x80000>;
				read-only;
			};

			partition@180000 {
				label = "ubifs";
				reg = <0x180000 0x1fe80000>;
			};
		};
	};
};
