/*
 * P1023/P1017 Silicon/SoC Device Tree Source (post include)
 *
 * Copyright 2011 Freescale Semiconductor Inc.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 *     * Redistributions of source code must retain the above copyright
 *       notice, this list of conditions and the following disclaimer.
 *     * Redistributions in binary form must reproduce the above copyright
 *       notice, this list of conditions and the following disclaimer in the
 *       documentation and/or other materials provided with the distribution.
 *     * Neither the name of Freescale Semiconductor nor the
 *       names of its contributors may be used to endorse or promote products
 *       derived from this software without specific prior written permission.
 *
 *
 * ALTERNATIVELY, this software may be distributed under the terms of the
 * GNU General Public License ("GPL") as published by the Free Software
 * Foundation, either version 2 of that License or (at your option) any
 * later version.
 *
 * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
 * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
 * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
 * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
 * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
 * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
 * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

&lbc {
	#address-cells = <2>;
	#size-cells = <1>;
	compatible = "fsl,p1023-elbc", "fsl,elbc", "simple-bus";
	interrupts = <19 2 0 0>,
		     <16 2 0 0>;
};

/* controller at 0xa000 */
&pci0 {
	compatible = "fsl,p1023-pcie", "fsl,qoriq-pcie-v2.2";
	device_type = "pci";
	#size-cells = <2>;
	#address-cells = <3>;
	bus-range = <0x0 0xff>;
	clock-frequency = <33333333>;
	interrupts = <16 2 0 0>;
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";
		interrupts = <16 2 0 0>;
	};
};

/* controller at 0x9000 */
&pci1 {
	compatible = "fsl,p1023-pcie", "fsl,qoriq-pcie-v2.2";
	device_type = "pci";
	#size-cells = <2>;
	#address-cells = <3>;
	bus-range = <0 0xff>;
	clock-frequency = <33333333>;
	interrupts = <16 2 0 0>;
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";
		interrupts = <16 2 0 0>;
	};
};

/* controller at 0xb000 */
&pci2 {
	compatible = "fsl,p1023-pcie", "fsl,qoriq-pcie-v2.2";
	device_type = "pci";
	#size-cells = <2>;
	#address-cells = <3>;
	bus-range = <0x0 0xff>;
	clock-frequency = <33333333>;
	interrupts = <16 2 0 0>;
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";
		interrupts = <16 2 0 0>;
	};
};

&soc {
	#address-cells = <1>;
	#size-cells = <1>;
	device_type = "soc";
	compatible = "fsl,p1023-immr", "simple-bus";
	bus-frequency = <0>;		// Filled out by uboot.

	ecm-law@0 {
		compatible = "fsl,ecm-law";
		reg = <0x0 0x1000>;
		fsl,num-laws = <12>;
	};

	ecm@1000 {
		compatible = "fsl,p1023-ecm", "fsl,ecm";
		reg = <0x1000 0x1000>;
		interrupts = <16 2 0 0>;
	};

	memory-controller@2000 {
		compatible = "fsl,p1023-memory-controller";
		reg = <0x2000 0x1000>;
		interrupts = <16 2 0 0>;
	};

/include/ "pq3-i2c-0.dtsi"
/include/ "pq3-i2c-1.dtsi"
/include/ "pq3-duart-0.dtsi"

/include/ "pq3-espi-0.dtsi"
	spi@7000 {
		fsl,espi-num-chipselects = <4>;
	};

/include/ "pq3-gpio-0.dtsi"

	L2: l2-cache-controller@20000 {
		compatible = "fsl,p1023-l2-cache-controller";
		reg = <0x20000 0x1000>;
		cache-line-size = <32>;	// 32 bytes
		cache-size = <0x40000>; // L2,256K
		interrupts = <16 2 0 0>;
	};

/include/ "pq3-dma-0.dtsi"
/include/ "pq3-usb2-dr-0.dtsi"
	usb@22000 {
		compatible = "fsl-usb2-dr-v1.6", "fsl-usb2-dr";
	};

	crypto: crypto@300000 {
		compatible = "fsl,sec-v4.2", "fsl,sec-v4.0";
		fsl,sec-era = <3>;
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0x30000 0x10000>;
		ranges = <0 0x30000 0x10000>;
		interrupts = <58 2 0 0>;

		sec_jr0: jr@1000 {
			compatible = "fsl,sec-v4.2-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg = <0x1000 0x1000>;
			interrupts = <45 2 0 0>;
		};

		sec_jr1: jr@2000 {
			compatible = "fsl,sec-v4.2-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg = <0x2000 0x1000>;
			interrupts = <45 2 0 0>;
		};

		sec_jr2: jr@3000 {
			compatible = "fsl,sec-v4.2-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg = <0x3000 0x1000>;
			interrupts = <57 2 0 0>;
		};

		sec_jr3: jr@4000 {
			compatible = "fsl,sec-v4.2-job-ring",
				     "fsl,sec-v4.0-job-ring";
			reg = <0x4000 0x1000>;
			interrupts = <57 2 0 0>;
		};

		rtic@6000 {
			compatible = "fsl,sec-v4.2-rtic",
				     "fsl,sec-v4.0-rtic";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x6000 0x100>;
			ranges = <0x0 0x6100 0xe00>;

			rtic_a: rtic-a@0 {
				compatible = "fsl,sec-v4.2-rtic-memory",
					     "fsl,sec-v4.0-rtic-memory";
				reg = <0x00 0x20 0x100 0x80>;
			};

			rtic_b: rtic-b@20 {
				compatible = "fsl,sec-v4.2-rtic-memory",
					     "fsl,sec-v4.0-rtic-memory";
				reg = <0x20 0x20 0x200 0x80>;
			};

			rtic_c: rtic-c@40 {
				compatible = "fsl,sec-v4.2-rtic-memory",
					     "fsl,sec-v4.0-rtic-memory";
				reg = <0x40 0x20 0x300 0x80>;
			};

			rtic_d: rtic-d@60 {
				compatible = "fsl,sec-v4.2-rtic-memory",
					     "fsl,sec-v4.0-rtic-memory";
				reg = <0x60 0x20 0x500 0x80>;
			};
		};
	};

/include/ "pq3-mpic.dtsi"
/include/ "pq3-mpic-timer-B.dtsi"

	global-utilities@e0000 {
		compatible = "fsl,p1023-guts";
		reg = <0xe0000 0x1000>;
		fsl,has-rstcr;
	};
};
