/*
 * Copyright 2012 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	memory {
		reg = <0x10000000 0x40000000>;
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_usb_otg_vbus: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "usb_otg_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio3 22 0>;
			enable-active-high;
		};

		reg_usb_h1_vbus: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "usb_h1_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio1 29 0>;
			enable-active-high;
		};

		reg_audio: regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "wm8962-supply";
			gpio = <&gpio4 10 0>;
			enable-active-high;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_gpio_keys>;

		power {
			label = "Power Button";
			gpios = <&gpio3 29 GPIO_ACTIVE_LOW>;
			gpio-key,wakeup;
			linux,code = <KEY_POWER>;
		};

		volume-up {
			label = "Volume Up";
			gpios = <&gpio1 4 GPIO_ACTIVE_LOW>;
			gpio-key,wakeup;
			linux,code = <KEY_VOLUMEUP>;
		};

		volume-down {
			label = "Volume Down";
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
			gpio-key,wakeup;
			linux,code = <KEY_VOLUMEDOWN>;
		};
	};

	sound {
		compatible = "fsl,imx6q-sabresd-wm8962",
			   "fsl,imx-audio-wm8962";
		model = "wm8962-audio";
		ssi-controller = <&ssi2>;
		audio-codec = <&codec>;
		audio-routing =
			"Headphone Jack", "HPOUTL",
			"Headphone Jack", "HPOUTR",
			"Ext Spk", "SPKOUTL",
			"Ext Spk", "SPKOUTR",
			"MICBIAS", "AMIC",
			"IN3R", "MICBIAS",
			"DMIC", "MICBIAS",
			"DMICDAT", "DMIC";
		mux-int-port = <2>;
		mux-ext-port = <3>;
	};

	backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 5000000>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <7>;
		status = "okay";
	};
};

&audmux {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_audmux>;
	status = "okay";
};

&ecspi1 {
	fsl,spi-num-chipselects = <1>;
	cs-gpios = <&gpio4 9 0>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_ecspi1>;
	status = "okay";

	flash: m25p80@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "st,m25p32";
		spi-max-frequency = <20000000>;
		reg = <0>;
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	phy-reset-gpios = <&gpio1 25 0>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	codec: wm8962@1a {
		compatible = "wlf,wm8962";
		reg = <0x1a>;
		clocks = <&clks 201>;
		DCVDD-supply = <&reg_audio>;
		DBVDD-supply = <&reg_audio>;
		AVDD-supply = <&reg_audio>;
		CPVDD-supply = <&reg_audio>;
		MICVDD-supply = <&reg_audio>;
		PLLVDD-supply = <&reg_audio>;
		SPKVDD1-supply = <&reg_audio>;
		SPKVDD2-supply = <&reg_audio>;
		gpio-cfg = <
			0x0000 /* 0:Default */
			0x0000 /* 1:Default */
			0x0013 /* 2:FN_DMICCLK */
			0x0000 /* 3:Default */
			0x8014 /* 4:FN_DMICCDAT */
			0x0000 /* 5:Default */
		>;
       };
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	pmic: pfuze100@08 {
		compatible = "fsl,pfuze100";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1c {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: sw4 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vgen1 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vgen3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";

	egalax_ts@04 {
		compatible = "eeti,egalax_ts";
		reg = <0x04>;
		interrupt-parent = <&gpio6>;
		interrupts = <7 2>;
		wakeup-gpios = <&gpio6 7 0>;
	};
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	imx6qdl-sabresd {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				MX6QDL_PAD_NANDF_D0__GPIO2_IO00 0x80000000
				MX6QDL_PAD_NANDF_D1__GPIO2_IO01 0x80000000
				MX6QDL_PAD_NANDF_D2__GPIO2_IO02 0x80000000
				MX6QDL_PAD_NANDF_D3__GPIO2_IO03 0x80000000
				MX6QDL_PAD_GPIO_0__CCM_CLKO1    0x130b0
				MX6QDL_PAD_NANDF_CLE__GPIO6_IO07 0x80000000
				MX6QDL_PAD_ENET_TXD1__GPIO1_IO29 0x80000000
				MX6QDL_PAD_EIM_D22__GPIO3_IO22  0x80000000
				MX6QDL_PAD_ENET_CRS_DV__GPIO1_IO25 0x80000000
			>;
		};

		pinctrl_audmux: audmuxgrp {
			fsl,pins = <
				MX6QDL_PAD_CSI0_DAT7__AUD3_RXD		0x130b0
				MX6QDL_PAD_CSI0_DAT4__AUD3_TXC		0x130b0
				MX6QDL_PAD_CSI0_DAT5__AUD3_TXD		0x110b0
				MX6QDL_PAD_CSI0_DAT6__AUD3_TXFS		0x130b0
			>;
		};

		pinctrl_ecspi1: ecspi1grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL1__ECSPI1_MISO	0x100b1
				MX6QDL_PAD_KEY_ROW0__ECSPI1_MOSI	0x100b1
				MX6QDL_PAD_KEY_COL0__ECSPI1_SCLK	0x100b1
			>;
		};

		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
			>;
		};

		pinctrl_gpio_keys: gpio_keysgrp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D29__GPIO3_IO29 0x80000000
				MX6QDL_PAD_GPIO_4__GPIO1_IO04  0x80000000
				MX6QDL_PAD_GPIO_5__GPIO1_IO05  0x80000000
			>;
		};

		pinctrl_i2c1: i2c1grp {
			fsl,pins = <
				MX6QDL_PAD_CSI0_DAT8__I2C1_SDA		0x4001b8b1
				MX6QDL_PAD_CSI0_DAT9__I2C1_SCL		0x4001b8b1
			>;
		};

		pinctrl_i2c2: i2c2grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b8b1
				MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b8b1
			>;
		};

		pinctrl_i2c3: i2c3grp {
			fsl,pins = <
				MX6QDL_PAD_GPIO_3__I2C3_SCL		0x4001b8b1
				MX6QDL_PAD_GPIO_6__I2C3_SDA		0x4001b8b1
			>;
		};

		pinctrl_pwm1: pwm1grp {
			fsl,pins = <
				MX6QDL_PAD_SD1_DAT3__PWM1_OUT		0x1b0b1
			>;
		};

		pinctrl_uart1: uart1grp {
			fsl,pins = <
				MX6QDL_PAD_CSI0_DAT10__UART1_TX_DATA	0x1b0b1
				MX6QDL_PAD_CSI0_DAT11__UART1_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_usbotg: usbotggrp {
			fsl,pins = <
				MX6QDL_PAD_ENET_RX_ER__USB_OTG_ID	0x17059
			>;
		};

		pinctrl_usdhc2: usdhc2grp {
			fsl,pins = <
				MX6QDL_PAD_SD2_CMD__SD2_CMD		0x17059
				MX6QDL_PAD_SD2_CLK__SD2_CLK		0x10059
				MX6QDL_PAD_SD2_DAT0__SD2_DATA0		0x17059
				MX6QDL_PAD_SD2_DAT1__SD2_DATA1		0x17059
				MX6QDL_PAD_SD2_DAT2__SD2_DATA2		0x17059
				MX6QDL_PAD_SD2_DAT3__SD2_DATA3		0x17059
				MX6QDL_PAD_NANDF_D4__SD2_DATA4		0x17059
				MX6QDL_PAD_NANDF_D5__SD2_DATA5		0x17059
				MX6QDL_PAD_NANDF_D6__SD2_DATA6		0x17059
				MX6QDL_PAD_NANDF_D7__SD2_DATA7		0x17059
			>;
		};

		pinctrl_usdhc3: usdhc3grp {
			fsl,pins = <
				MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17059
				MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10059
				MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
				MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
				MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
				MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
				MX6QDL_PAD_SD3_DAT4__SD3_DATA4		0x17059
				MX6QDL_PAD_SD3_DAT5__SD3_DATA5		0x17059
				MX6QDL_PAD_SD3_DAT6__SD3_DATA6		0x17059
				MX6QDL_PAD_SD3_DAT7__SD3_DATA7		0x17059
			>;
		};
	};
};

&ldb {
	status = "okay";

	lvds-channel@1 {
		fsl,data-mapping = "spwg";
		fsl,data-width = <18>;
		status = "okay";

		display-timings {
			native-mode = <&timing0>;
			timing0: hsd100pxn1 {
				clock-frequency = <65000000>;
				hactive = <1024>;
				vactive = <768>;
				hback-porch = <220>;
				hfront-porch = <40>;
				vback-porch = <21>;
				vfront-porch = <7>;
				hsync-len = <60>;
				vsync-len = <10>;
			};
		};
	};
};

&pwm1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>;
	status = "okay";
};

&ssi2 {
	fsl,mode = "i2s-slave";
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&usbh1 {
	vbus-supply = <&reg_usb_h1_vbus>;
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_usb_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	disable-over-current;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2>;
	bus-width = <8>;
	cd-gpios = <&gpio2 2 0>;
	wp-gpios = <&gpio2 3 0>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	bus-width = <8>;
	cd-gpios = <&gpio2 0 0>;
	wp-gpios = <&gpio2 1 0>;
	status = "okay";
};
