/*
 * PQ3 Sec/Crypto 4.4 device tree stub [ controller @ offset 0x30000 ]
 *
 * Copyright 2011 Freescale Semiconductor Inc.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 *     * Redistributions of source code must retain the above copyright
 *       notice, this list of conditions and the following disclaimer.
 *     * Redistributions in binary form must reproduce the above copyright
 *       notice, this list of conditions and the following disclaimer in the
 *       documentation and/or other materials provided with the distribution.
 *     * Neither the name of Freescale Semiconductor nor the
 *       names of its contributors may be used to endorse or promote products
 *       derived from this software without specific prior written permission.
 *
 *
 * ALTERNATIVELY, this software may be distributed under the terms of the
 * GNU General Public License ("GPL") as published by the Free Software
 * Foundation, either version 2 of that License or (at your option) any
 * later version.
 *
 * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
 * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
 * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
 * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
 * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
 * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
 * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
 * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
 * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

crypto@30000 {
	compatible = "fsl,sec-v4.4", "fsl,sec-v4.0";
	fsl,sec-era = <3>;
	#address-cells = <1>;
	#size-cells = <1>;
	ranges		 = <0x0 0x30000 0x10000>;
	reg		 = <0x30000 0x10000>;
	interrupts	 = <58 2 0 0>;

	sec_jr0: jr@1000 {
		compatible = "fsl,sec-v4.4-job-ring", "fsl,sec-v4.0-job-ring";
		reg	   = <0x1000 0x1000>;
		interrupts	 = <45 2 0 0>;
	};

	sec_jr1: jr@2000 {
		compatible = "fsl,sec-v4.4-job-ring", "fsl,sec-v4.0-job-ring";
		reg	   = <0x2000 0x1000>;
		interrupts	 = <45 2 0 0>;
	};

	sec_jr2: jr@3000 {
		compatible = "fsl,sec-v4.4-job-ring", "fsl,sec-v4.0-job-ring";
		reg	   = <0x3000 0x1000>;
		interrupts	 = <45 2 0 0>;
	};

	sec_jr3: jr@4000 {
		compatible = "fsl,sec-v4.4-job-ring", "fsl,sec-v4.0-job-ring";
		reg	   = <0x4000 0x1000>;
		interrupts	 = <45 2 0 0>;
	};
};
