/*
 * FriendlyARM's Exynos4412 based TINY4412 board device tree source
 *
 * Copyright (c) 2013 Alex Ling <kasimling@gmail.com>
 *
 * Device tree source file for FriendlyARM's TINY4412 board which is based on
 * Samsung's Exynos4412 SoC.
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
*/

/dts-v1/;
#include "exynos4412.dtsi"

/ {
	model = "FriendlyARM TINY4412 board based on Exynos4412";
	compatible = "friendlyarm,tiny4412", "samsung,exynos4412", "samsung,exynos4";

	memory {
		reg = <0x40000000 0x40000000>;
	};

	leds {
		compatible = "gpio-leds";

		led1 {
			label = "led1";
			gpios = <&gpm4 0 1>;
			default-state = "off";
			linux,default-trigger = "heartbeat";
		};

		led2 {
			label = "led2";
			gpios = <&gpm4 1 1>;
			default-state = "off";
		};

		led3 {
			label = "led3";
			gpios = <&gpm4 2 1>;
			default-state = "off";
		};

		led4 {
			label = "led4";
			gpios = <&gpm4 3 1>;
			default-state = "off";
			linux,default-trigger = "mmc0";
		};
	};

	rtc@10070000 {
		status = "okay";
	};

	sdhci@12530000 {
		bus-width = <4>;
		pinctrl-0 = <&sd2_clk &sd2_cmd &sd2_cd &sd2_bus4>;
		pinctrl-names = "default";
		status = "okay";
	};

	serial@13800000 {
		status = "okay";
	};

	serial@13810000 {
		status = "okay";
	};

	serial@13820000 {
		status = "okay";
	};

	serial@13830000 {
		status = "okay";
	};

	fixed-rate-clocks {
		xxti {
			compatible = "samsung,clock-xxti";
			clock-frequency = <0>;
		};

		xusbxti {
			compatible = "samsung,clock-xusbxti";
			clock-frequency = <24000000>;
		};
	};
};
