/*
 * Copyright 2012 Linaro Ltd
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/mfd/dbx500-prcmu.h>
#include "skeleton.dtsi"

/ {
	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "stericsson,db8500";
		interrupt-parent = <&intc>;
		ranges;

		intc: interrupt-controller@a0411000 {
			compatible = "arm,cortex-a9-gic";
			#interrupt-cells = <3>;
			#address-cells = <1>;
			interrupt-controller;
			reg = <0xa0411000 0x1000>,
			      <0xa0410100 0x100>;
		};

		L2: l2-cache {
			compatible = "arm,pl310-cache";
			reg = <0xa0412000 0x1000>;
			interrupts = <0 13 IRQ_TYPE_LEVEL_HIGH>;
			cache-unified;
			cache-level = <2>;
		};

		pmu {
			compatible = "arm,cortex-a9-pmu";
			interrupts = <0 7 IRQ_TYPE_LEVEL_HIGH>;
		};


		clocks {
			compatible = "stericsson,u8500-clks";

			prcmu_clk: prcmu-clock {
				#clock-cells = <1>;
			};

			prcc_pclk: prcc-periph-clock {
				#clock-cells = <2>;
			};

			prcc_kclk: prcc-kernel-clock {
				#clock-cells = <2>;
			};

			rtc_clk: rtc32k-clock {
				#clock-cells = <0>;
			};

			smp_twd_clk: smp-twd-clock {
				#clock-cells = <0>;
			};
		};

		mtu@a03c6000 {
			/* Nomadik System Timer */
			compatible = "st,nomadik-mtu";
			reg = <0xa03c6000 0x1000>;
			interrupts = <0 4 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&prcmu_clk PRCMU_TIMCLK>, <&prcc_pclk 6 6>;
			clock-names = "timclk", "apb_pclk";
		};

		timer@a0410600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0xa0410600 0x20>;
			interrupts = <1 13 0x304>; /* IRQ level high per-CPU */

			clocks = <&smp_twd_clk>;
		};

		rtc@80154000 {
			compatible = "arm,rtc-pl031", "arm,primecell";
			reg = <0x80154000 0x1000>;
			interrupts = <0 18 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&rtc_clk>;
			clock-names = "apb_pclk";
		};

		gpio0: gpio@8012e000 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8012e000 0x80>;
			interrupts = <0 119 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <0>;

			clocks = <&prcc_pclk 1 9>;
		};

		gpio1: gpio@8012e080 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8012e080 0x80>;
			interrupts = <0 120 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <1>;

			clocks = <&prcc_pclk 1 9>;
		};

		gpio2: gpio@8000e000 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8000e000 0x80>;
			interrupts = <0 121 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <2>;

			clocks = <&prcc_pclk 3 8>;
		};

		gpio3: gpio@8000e080 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8000e080 0x80>;
			interrupts = <0 122 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <3>;

			clocks = <&prcc_pclk 3 8>;
		};

		gpio4: gpio@8000e100 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8000e100 0x80>;
			interrupts = <0 123 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <4>;

			clocks = <&prcc_pclk 3 8>;
		};

		gpio5: gpio@8000e180 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8000e180 0x80>;
			interrupts = <0 124 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <5>;

			clocks = <&prcc_pclk 3 8>;
		};

		gpio6: gpio@8011e000 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8011e000 0x80>;
			interrupts = <0 125 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <6>;

			clocks = <&prcc_pclk 2 11>;
		};

		gpio7: gpio@8011e080 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0x8011e080 0x80>;
			interrupts = <0 126 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <7>;

			clocks = <&prcc_pclk 2 11>;
		};

		gpio8: gpio@a03fe000 {
			compatible = "stericsson,db8500-gpio",
				"st,nomadik-gpio";
			reg =  <0xa03fe000 0x80>;
			interrupts = <0 127 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			st,supports-sleepmode;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-bank = <8>;

			clocks = <&prcc_pclk 5 1>;
		};

		pinctrl {
			compatible = "stericsson,db8500-pinctrl";
			prcm = <&prcmu>;
		};

		usb_per5@a03e0000 {
			compatible = "stericsson,db8500-musb";
			reg = <0xa03e0000 0x10000>;
			interrupts = <0 23 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "mc";

			dr_mode = "otg";

			dmas = <&dma 38 0 0x2>, /* Logical - DevToMem */
			       <&dma 38 0 0x0>, /* Logical - MemToDev */
			       <&dma 37 0 0x2>, /* Logical - DevToMem */
			       <&dma 37 0 0x0>, /* Logical - MemToDev */
			       <&dma 36 0 0x2>, /* Logical - DevToMem */
			       <&dma 36 0 0x0>, /* Logical - MemToDev */
			       <&dma 19 0 0x2>, /* Logical - DevToMem */
			       <&dma 19 0 0x0>, /* Logical - MemToDev */
			       <&dma 18 0 0x2>, /* Logical - DevToMem */
			       <&dma 18 0 0x0>, /* Logical - MemToDev */
			       <&dma 17 0 0x2>, /* Logical - DevToMem */
			       <&dma 17 0 0x0>, /* Logical - MemToDev */
			       <&dma 16 0 0x2>, /* Logical - DevToMem */
			       <&dma 16 0 0x0>, /* Logical - MemToDev */
			       <&dma 39 0 0x2>, /* Logical - DevToMem */
			       <&dma 39 0 0x0>; /* Logical - MemToDev */

			dma-names = "iep_1_9",  "oep_1_9",
				    "iep_2_10", "oep_2_10",
				    "iep_3_11", "oep_3_11",
				    "iep_4_12", "oep_4_12",
				    "iep_5_13", "oep_5_13",
				    "iep_6_14", "oep_6_14",
				    "iep_7_15", "oep_7_15",
				    "iep_8",    "oep_8";

			clocks = <&prcc_pclk 5 0>;
		};

		dma: dma-controller@801C0000 {
			compatible = "stericsson,db8500-dma40", "stericsson,dma40";
			reg = <0x801C0000 0x1000 0x40010000 0x800>;
			reg-names = "base", "lcpa";
			interrupts = <0 25 IRQ_TYPE_LEVEL_HIGH>;

			#dma-cells = <3>;
			memcpy-channels = <56 57 58 59 60>;

			clocks = <&prcmu_clk PRCMU_DMACLK>;
		};

		prcmu: prcmu@80157000 {
			compatible = "stericsson,db8500-prcmu";
			reg = <0x80157000 0x2000>, <0x801b0000 0x8000>, <0x801b8000 0x1000>;
			reg-names = "prcmu", "prcmu-tcpm", "prcmu-tcdm";
			interrupts = <0 47 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <1>;
			interrupt-controller;
			#interrupt-cells = <2>;
			ranges;

			prcmu-timer-4@80157450 {
				compatible = "stericsson,db8500-prcmu-timer-4";
				reg = <0x80157450 0xC>;
			};

			cpufreq {
				compatible = "stericsson,cpufreq-ux500";
				clocks = <&prcmu_clk PRCMU_ARMSS>;
				clock-names = "armss";
				status = "disabled";
			};

			thermal@801573c0 {
				compatible = "stericsson,db8500-thermal";
				reg = <0x801573c0 0x40>;
				interrupts = <21 IRQ_TYPE_LEVEL_HIGH>,
					     <22 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "IRQ_HOTMON_LOW", "IRQ_HOTMON_HIGH";
				status = "disabled";
			};

			db8500-prcmu-regulators {
				compatible = "stericsson,db8500-prcmu-regulator";

				// DB8500_REGULATOR_VAPE
				db8500_vape_reg: db8500_vape {
					regulator-compatible = "db8500_vape";
					regulator-always-on;
				};

				// DB8500_REGULATOR_VARM
				db8500_varm_reg: db8500_varm {
					regulator-compatible = "db8500_varm";
				};

				// DB8500_REGULATOR_VMODEM
				db8500_vmodem_reg: db8500_vmodem {
					regulator-compatible = "db8500_vmodem";
				};

				// DB8500_REGULATOR_VPLL
				db8500_vpll_reg: db8500_vpll {
					regulator-compatible = "db8500_vpll";
				};

				// DB8500_REGULATOR_VSMPS1
				db8500_vsmps1_reg: db8500_vsmps1 {
					regulator-compatible = "db8500_vsmps1";
				};

				// DB8500_REGULATOR_VSMPS2
				db8500_vsmps2_reg: db8500_vsmps2 {
					regulator-compatible = "db8500_vsmps2";
				};

				// DB8500_REGULATOR_VSMPS3
				db8500_vsmps3_reg: db8500_vsmps3 {
					regulator-compatible = "db8500_vsmps3";
				};

				// DB8500_REGULATOR_VRF1
				db8500_vrf1_reg: db8500_vrf1 {
					regulator-compatible = "db8500_vrf1";
				};

				// DB8500_REGULATOR_SWITCH_SVAMMDSP
				db8500_sva_mmdsp_reg: db8500_sva_mmdsp {
					regulator-compatible = "db8500_sva_mmdsp";
				};

				// DB8500_REGULATOR_SWITCH_SVAMMDSPRET
				db8500_sva_mmdsp_ret_reg: db8500_sva_mmdsp_ret {
					regulator-compatible = "db8500_sva_mmdsp_ret";
				};

				// DB8500_REGULATOR_SWITCH_SVAPIPE
				db8500_sva_pipe_reg: db8500_sva_pipe {
					regulator-compatible = "db8500_sva_pipe";
				};

				// DB8500_REGULATOR_SWITCH_SIAMMDSP
				db8500_sia_mmdsp_reg: db8500_sia_mmdsp {
					regulator-compatible = "db8500_sia_mmdsp";
				};

				// DB8500_REGULATOR_SWITCH_SIAMMDSPRET
				db8500_sia_mmdsp_ret_reg: db8500_sia_mmdsp_ret {
				};

				// DB8500_REGULATOR_SWITCH_SIAPIPE
				db8500_sia_pipe_reg: db8500_sia_pipe {
					regulator-compatible = "db8500_sia_pipe";
				};

				// DB8500_REGULATOR_SWITCH_SGA
				db8500_sga_reg: db8500_sga {
					regulator-compatible = "db8500_sga";
					vin-supply = <&db8500_vape_reg>;
				};

				// DB8500_REGULATOR_SWITCH_B2R2_MCDE
				db8500_b2r2_mcde_reg: db8500_b2r2_mcde {
					regulator-compatible = "db8500_b2r2_mcde";
					vin-supply = <&db8500_vape_reg>;
				};

				// DB8500_REGULATOR_SWITCH_ESRAM12
				db8500_esram12_reg: db8500_esram12 {
					regulator-compatible = "db8500_esram12";
				};

				// DB8500_REGULATOR_SWITCH_ESRAM12RET
				db8500_esram12_ret_reg: db8500_esram12_ret {
					regulator-compatible = "db8500_esram12_ret";
				};

				// DB8500_REGULATOR_SWITCH_ESRAM34
				db8500_esram34_reg: db8500_esram34 {
					regulator-compatible = "db8500_esram34";
				};

				// DB8500_REGULATOR_SWITCH_ESRAM34RET
				db8500_esram34_ret_reg: db8500_esram34_ret {
					regulator-compatible = "db8500_esram34_ret";
				};
			};

			ab8500 {
				compatible = "stericsson,ab8500";
				interrupt-parent = <&intc>;
				interrupts = <0 40 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				ab8500_gpio: ab8500-gpio {
					gpio-controller;
					#gpio-cells = <2>;
				};

				ab8500-rtc {
					compatible = "stericsson,ab8500-rtc";
					interrupts = <17 IRQ_TYPE_LEVEL_HIGH
						      18 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "60S", "ALARM";
				};

				ab8500-gpadc {
					compatible = "stericsson,ab8500-gpadc";
					interrupts = <32 IRQ_TYPE_LEVEL_HIGH
						      39 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "HW_CONV_END", "SW_CONV_END";
					vddadc-supply = <&ab8500_ldo_tvout_reg>;
				};

				ab8500_battery: ab8500_battery {
					stericsson,battery-type = "LIPO";
					thermistor-on-batctrl;
				};

				ab8500_fg {
					compatible = "stericsson,ab8500-fg";
					battery	   = <&ab8500_battery>;
				};

				ab8500_btemp {
					compatible = "stericsson,ab8500-btemp";
					battery	   = <&ab8500_battery>;
				};

				ab8500_charger {
					compatible	= "stericsson,ab8500-charger";
					battery		= <&ab8500_battery>;
					vddadc-supply	= <&ab8500_ldo_tvout_reg>;
				};

				ab8500_chargalg {
					compatible	= "stericsson,ab8500-chargalg";
					battery		= <&ab8500_battery>;
				};

				ab8500_usb {
					compatible = "stericsson,ab8500-usb";
					interrupts = < 90 IRQ_TYPE_LEVEL_HIGH
						       96 IRQ_TYPE_LEVEL_HIGH
						       14 IRQ_TYPE_LEVEL_HIGH
						       15 IRQ_TYPE_LEVEL_HIGH
						       79 IRQ_TYPE_LEVEL_HIGH
						       74 IRQ_TYPE_LEVEL_HIGH
						       75 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "ID_WAKEUP_R",
							  "ID_WAKEUP_F",
							  "VBUS_DET_F",
							  "VBUS_DET_R",
							  "USB_LINK_STATUS",
							  "USB_ADP_PROBE_PLUG",
							  "USB_ADP_PROBE_UNPLUG";
					vddulpivio18-supply = <&ab8500_ldo_intcore_reg>;
					v-ape-supply = <&db8500_vape_reg>;
					musb_1v8-supply = <&db8500_vsmps2_reg>;
				};

				ab8500-ponkey {
					compatible = "stericsson,ab8500-poweron-key";
					interrupts = <6 IRQ_TYPE_LEVEL_HIGH
						      7 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "ONKEY_DBF", "ONKEY_DBR";
				};

				ab8500-sysctrl {
					compatible = "stericsson,ab8500-sysctrl";
				};

				ab8500-pwm {
					compatible = "stericsson,ab8500-pwm";
				};

				ab8500-debugfs {
					compatible = "stericsson,ab8500-debug";
				};

				codec: ab8500-codec {
					compatible = "stericsson,ab8500-codec";

					V-AUD-supply = <&ab8500_ldo_audio_reg>;
					V-AMIC1-supply = <&ab8500_ldo_anamic1_reg>;
					V-AMIC2-supply = <&ab8500_ldo_anamic2_reg>;
					V-DMIC-supply = <&ab8500_ldo_dmic_reg>;

					stericsson,earpeice-cmv = <950>; /* Units in mV. */
				};

				ext_regulators: ab8500-ext-regulators {
					compatible = "stericsson,ab8500-ext-regulator";

					ab8500_ext1_reg: ab8500_ext1 {
						regulator-compatible = "ab8500_ext1";
						regulator-min-microvolt = <1800000>;
						regulator-max-microvolt = <1800000>;
						regulator-boot-on;
						regulator-always-on;
					};

					ab8500_ext2_reg: ab8500_ext2 {
						regulator-compatible = "ab8500_ext2";
						regulator-min-microvolt = <1360000>;
						regulator-max-microvolt = <1360000>;
						regulator-boot-on;
						regulator-always-on;
					};

					ab8500_ext3_reg: ab8500_ext3 {
						regulator-compatible = "ab8500_ext3";
						regulator-min-microvolt = <3400000>;
						regulator-max-microvolt = <3400000>;
						regulator-boot-on;
					};
				};

				ab8500-regulators {
					compatible = "stericsson,ab8500-regulator";
					vin-supply = <&ab8500_ext3_reg>;

					// supplies to the display/camera
					ab8500_ldo_aux1_reg: ab8500_ldo_aux1 {
						regulator-compatible = "ab8500_ldo_aux1";
						regulator-min-microvolt = <2500000>;
						regulator-max-microvolt = <2900000>;
						regulator-boot-on;
						/* BUG: If turned off MMC will be affected. */
						regulator-always-on;
					};

					// supplies to the on-board eMMC
					ab8500_ldo_aux2_reg: ab8500_ldo_aux2 {
						regulator-compatible = "ab8500_ldo_aux2";
						regulator-min-microvolt = <1100000>;
						regulator-max-microvolt = <3300000>;
					};

					// supply for VAUX3; SDcard slots
					ab8500_ldo_aux3_reg: ab8500_ldo_aux3 {
						regulator-compatible = "ab8500_ldo_aux3";
						regulator-min-microvolt = <1100000>;
						regulator-max-microvolt = <3300000>;
					};

					// supply for v-intcore12; VINTCORE12 LDO
					ab8500_ldo_intcore_reg: ab8500_ldo_intcore {
						regulator-compatible = "ab8500_ldo_intcore";
					};

					// supply for tvout; gpadc; TVOUT LDO
					ab8500_ldo_tvout_reg: ab8500_ldo_tvout {
						regulator-compatible = "ab8500_ldo_tvout";
					};

					// supply for ab8500-usb; USB LDO
					ab8500_ldo_usb_reg: ab8500_ldo_usb {
						regulator-compatible = "ab8500_ldo_usb";
					};

					// supply for ab8500-vaudio; VAUDIO LDO
					ab8500_ldo_audio_reg: ab8500_ldo_audio {
						regulator-compatible = "ab8500_ldo_audio";
					};

					// supply for v-anamic1 VAMIC1 LDO
					ab8500_ldo_anamic1_reg: ab8500_ldo_anamic1 {
						regulator-compatible = "ab8500_ldo_anamic1";
					};

					// supply for v-amic2; VAMIC2 LDO; reuse constants for AMIC1
					ab8500_ldo_anamic2_reg: ab8500_ldo_anamic2 {
						regulator-compatible = "ab8500_ldo_anamic2";
					};

					// supply for v-dmic; VDMIC LDO
					ab8500_ldo_dmic_reg: ab8500_ldo_dmic {
						regulator-compatible = "ab8500_ldo_dmic";
					};

					// supply for U8500 CSI/DSI; VANA LDO
					ab8500_ldo_ana_reg: ab8500_ldo_ana {
						regulator-compatible = "ab8500_ldo_ana";
					};
				};
			};
		};

		i2c@80004000 {
			compatible = "stericsson,db8500-i2c", "st,nomadik-i2c", "arm,primecell";
			reg = <0x80004000 0x1000>;
			interrupts = <0 21 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;
			v-i2c-supply = <&db8500_vape_reg>;

			clock-frequency = <400000>;
			clocks = <&prcc_kclk 3 3>, <&prcc_pclk 3 3>;
			clock-names = "i2cclk", "apb_pclk";
		};

		i2c@80122000 {
			compatible = "stericsson,db8500-i2c", "st,nomadik-i2c", "arm,primecell";
			reg = <0x80122000 0x1000>;
			interrupts = <0 22 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;
			v-i2c-supply = <&db8500_vape_reg>;

			clock-frequency = <400000>;

			clocks = <&prcc_kclk 1 2>, <&prcc_pclk 1 2>;
			clock-names = "i2cclk", "apb_pclk";
		};

		i2c@80128000 {
			compatible = "stericsson,db8500-i2c", "st,nomadik-i2c", "arm,primecell";
			reg = <0x80128000 0x1000>;
			interrupts = <0 55 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;
			v-i2c-supply = <&db8500_vape_reg>;

			clock-frequency = <400000>;

			clocks = <&prcc_kclk 1 6>, <&prcc_pclk 1 6>;
			clock-names = "i2cclk", "apb_pclk";
		};

		i2c@80110000 {
			compatible = "stericsson,db8500-i2c", "st,nomadik-i2c", "arm,primecell";
			reg = <0x80110000 0x1000>;
			interrupts = <0 12 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;
			v-i2c-supply = <&db8500_vape_reg>;

			clock-frequency = <400000>;

			clocks = <&prcc_kclk 2 0>, <&prcc_pclk 2 0>;
			clock-names = "i2cclk", "apb_pclk";
		};

		i2c@8012a000 {
			compatible = "stericsson,db8500-i2c", "st,nomadik-i2c", "arm,primecell";
			reg = <0x8012a000 0x1000>;
			interrupts = <0 51 IRQ_TYPE_LEVEL_HIGH>;

			#address-cells = <1>;
			#size-cells = <0>;
			v-i2c-supply = <&db8500_vape_reg>;

			clock-frequency = <400000>;

			clocks = <&prcc_kclk 1 9>, <&prcc_pclk 1 10>;
			clock-names = "i2cclk", "apb_pclk";
		};

		ssp@80002000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x80002000 0x1000>;
			interrupts = <0 14 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&prcc_kclk 3 1>, <&prcc_pclk 3 1>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 8 0 0x2>, /* Logical - DevToMem */
			       <&dma 8 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		ssp@80003000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x80003000 0x1000>;
			interrupts = <0 52 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&prcc_kclk 3 2>, <&prcc_pclk 3 2>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 9 0 0x2>, /* Logical - DevToMem */
			       <&dma 9 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		spi@8011a000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x8011a000 0x1000>;
			interrupts = <0 8 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			/* Same clock wired to kernel and pclk */
			clocks = <&prcc_pclk 2 8>, <&prcc_pclk 2 8>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 0 0 0x2>, /* Logical - DevToMem */
			       <&dma 0 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		spi@80112000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x80112000 0x1000>;
			interrupts = <0 96 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			/* Same clock wired to kernel and pclk */
			clocks = <&prcc_pclk 2 2>, <&prcc_pclk 2 2>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 35 0 0x2>, /* Logical - DevToMem */
			       <&dma 35 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		spi@80111000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x80111000 0x1000>;
			interrupts = <0 6 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			/* Same clock wired to kernel and pclk */
			clocks = <&prcc_pclk 2 1>, <&prcc_pclk 2 1>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 33 0 0x2>, /* Logical - DevToMem */
			       <&dma 33 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		spi@80129000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x80129000 0x1000>;
			interrupts = <0 49 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			/* Same clock wired to kernel and pclk */
			clocks = <&prcc_pclk 1 7>, <&prcc_pclk 1 7>;
			clock-names = "SSPCLK", "apb_pclk";
			dmas = <&dma 40 0 0x2>, /* Logical - DevToMem */
			       <&dma 40 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";
		};

		uart@80120000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x80120000 0x1000>;
			interrupts = <0 11 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 13 0 0x2>, /* Logical - DevToMem */
			       <&dma 13 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 1 0>, <&prcc_pclk 1 0>;
			clock-names = "uart", "apb_pclk";

			status = "disabled";
		};

		uart@80121000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x80121000 0x1000>;
			interrupts = <0 19 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 12 0 0x2>, /* Logical - DevToMem */
			       <&dma 12 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 1 1>, <&prcc_pclk 1 1>;
			clock-names = "uart", "apb_pclk";

			status = "disabled";
		};

		uart@80007000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x80007000 0x1000>;
			interrupts = <0 26 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 11 0 0x2>, /* Logical - DevToMem */
			       <&dma 11 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 3 6>, <&prcc_pclk 3 6>;
			clock-names = "uart", "apb_pclk";

			status = "disabled";
		};

		sdi0_per1@80126000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80126000 0x1000>;
			interrupts = <0 60 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 29 0 0x2>, /* Logical - DevToMem */
			       <&dma 29 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 1 5>, <&prcc_pclk 1 5>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		sdi1_per2@80118000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80118000 0x1000>;
			interrupts = <0 50 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 32 0 0x2>, /* Logical - DevToMem */
			       <&dma 32 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 2 4>, <&prcc_pclk 2 6>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		sdi2_per3@80005000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80005000 0x1000>;
			interrupts = <0 41 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 28 0 0x2>, /* Logical - DevToMem */
			       <&dma 28 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 3 4>, <&prcc_pclk 3 4>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		sdi3_per2@80119000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80119000 0x1000>;
			interrupts = <0 59 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&prcc_kclk 2 5>, <&prcc_pclk 2 7>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		sdi4_per2@80114000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80114000 0x1000>;
			interrupts = <0 99 IRQ_TYPE_LEVEL_HIGH>;

			dmas = <&dma 42 0 0x2>, /* Logical - DevToMem */
			       <&dma 42 0 0x0>; /* Logical - MemToDev */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 2 2>, <&prcc_pclk 2 4>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		sdi5_per3@80008000 {
			compatible = "arm,pl18x", "arm,primecell";
			reg = <0x80008000 0x1000>;
			interrupts = <0 100 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&prcc_kclk 3 7>, <&prcc_pclk 3 7>;
			clock-names = "sdi", "apb_pclk";

			status = "disabled";
		};

		msp0: msp@80123000 {
			compatible = "stericsson,ux500-msp-i2s";
			reg = <0x80123000 0x1000>;
			interrupts = <0 31 IRQ_TYPE_LEVEL_HIGH>;
			v-ape-supply = <&db8500_vape_reg>;

			dmas = <&dma 31 0 0x12>, /* Logical - DevToMem - HighPrio */
			       <&dma 31 0 0x10>; /* Logical - MemToDev - HighPrio */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 1 3>, <&prcc_pclk 1 3>;
			clock-names = "msp", "apb_pclk";

			status = "disabled";
		};

		msp1: msp@80124000 {
			compatible = "stericsson,ux500-msp-i2s";
			reg = <0x80124000 0x1000>;
			interrupts = <0 62 IRQ_TYPE_LEVEL_HIGH>;
			v-ape-supply = <&db8500_vape_reg>;

			dmas = <&dma 30 0 0x10>; /* Logical - MemToDev - HighPrio */
			dma-names = "tx";

			clocks = <&prcc_kclk 1 4>, <&prcc_pclk 1 4>;
			clock-names = "msp", "apb_pclk";

			status = "disabled";
		};

		// HDMI sound
		msp2: msp@80117000 {
			compatible = "stericsson,ux500-msp-i2s";
			reg = <0x80117000 0x1000>;
			interrupts = <0 98 IRQ_TYPE_LEVEL_HIGH>;
			v-ape-supply = <&db8500_vape_reg>;

			dmas = <&dma 14 0 0x12>, /* Logical  - DevToMem - HighPrio */
			       <&dma 14 1 0x19>; /* Physical Chan 1 - MemToDev
                                                    HighPrio - Fixed */
			dma-names = "rx", "tx";

			clocks = <&prcc_kclk 2 3>, <&prcc_pclk 2 5>;
			clock-names = "msp", "apb_pclk";

			status = "disabled";
		};

		msp3: msp@80125000 {
			compatible = "stericsson,ux500-msp-i2s";
			reg = <0x80125000 0x1000>;
			interrupts = <0 62 IRQ_TYPE_LEVEL_HIGH>;
			v-ape-supply = <&db8500_vape_reg>;

			dmas = <&dma 30 0 0x12>; /* Logical - DevToMem - HighPrio */
			dma-names = "rx";

			clocks = <&prcc_kclk 1 10>, <&prcc_pclk 1 11>;
			clock-names = "msp", "apb_pclk";

			status = "disabled";
		};

		external-bus@50000000 {
			compatible = "simple-bus";
			reg = <0x50000000 0x4000000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x50000000 0x4000000>;
			status = "disabled";
		};

		cpufreq-cooling {
			compatible = "stericsson,db8500-cpufreq-cooling";
			status = "disabled";
		};

		vmmci: regulator-gpio {
			compatible = "regulator-gpio";

			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <2900000>;
			regulator-name = "mmci-reg";
			regulator-type = "voltage";

			startup-delay-us = <100>;
			enable-active-high;

			states = <1800000 0x1
				  2900000 0x0>;

			status = "disabled";
		};

		mcde@a0350000 {
			compatible = "stericsson,mcde";
			reg = <0xa0350000 0x1000>, /* MCDE */
			      <0xa0351000 0x1000>, /* DSI link 1 */
			      <0xa0352000 0x1000>, /* DSI link 2 */
			      <0xa0353000 0x1000>; /* DSI link 3 */
			interrupts = <0 48 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&prcmu_clk PRCMU_MCDECLK>, /* Main MCDE clock */
				 <&prcmu_clk PRCMU_LCDCLK>, /* LCD clock */
				 <&prcmu_clk PRCMU_PLLDSI>, /* HDMI clock */
				 <&prcmu_clk PRCMU_DSI0CLK>, /* DSI 0 */
				 <&prcmu_clk PRCMU_DSI1CLK>, /* DSI 1 */
				 <&prcmu_clk PRCMU_DSI0ESCCLK>, /* TVout clock 0 */
				 <&prcmu_clk PRCMU_DSI1ESCCLK>, /* TVout clock 1 */
				 <&prcmu_clk PRCMU_DSI2ESCCLK>; /* TVout clock 2 */
		};

		cryp@a03cb000 {
			compatible = "stericsson,ux500-cryp";
			reg = <0xa03cb000 0x1000>;
			interrupts = <0 15 IRQ_TYPE_LEVEL_HIGH>;

			v-ape-supply = <&db8500_vape_reg>;
			clocks = <&prcc_pclk 6 1>;
		};

		hash@a03c2000 {
			compatible = "stericsson,ux500-hash";
			reg = <0xa03c2000 0x1000>;

			v-ape-supply = <&db8500_vape_reg>;
			clocks = <&prcc_pclk 6 2>;
		};
	};
};
