/*
 * Copyright 2013 Maxime Ripard
 *
 * Maxime Ripard <maxime.ripard@free-electrons.com>
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
/include/ "sun6i-a31.dtsi"

/ {
	model = "WITS A31 Colombus Evaluation Board";
	compatible = "wits,colombus", "allwinner,sun6i-a31";

	chosen {
		bootargs = "earlyprintk console=ttyS0,115200";
	};

	soc@01c00000 {
		uart0: serial@01c28000 {
			pinctrl-names = "default";
			pinctrl-0 = <&uart0_pins_a>;
			status = "okay";
		};

		i2c0: i2c@01c2ac00 {
			pinctrl-names = "default";
			pinctrl-0 = <&i2c0_pins_a>;
			status = "fail";
		};

		i2c1: i2c@01c2b000 {
			pinctrl-names = "default";
			pinctrl-0 = <&i2c1_pins_a>;
			status = "okay";
		};

		i2c2: i2c@01c2b400 {
			pinctrl-names = "default";
			pinctrl-0 = <&i2c2_pins_a>;
			status = "okay";
		};
	};
};
