/*
 * Copyright (c) 2013 Heiko Stuebner <heiko@sntech.de>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License as published by
 * the Free Software Foundation; either version 2 of the License, or
 * (at your option) any later version.
 *
 * This program is distributed in the hope that it will be useful,
 * but WITHOUT ANY WARRANTY; without even the implied warranty of
 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 * GNU General Public License for more details.
 */

/dts-v1/;
#include "rk3188.dtsi"

/ {
	model = "Radxa Rock";
	compatible = "radxa,rock", "rockchip,rk3188";

	memory {
		reg = <0x60000000 0x80000000>;
	};

	soc {
		uart2: serial@20064000 {
			pinctrl-names = "default";
			pinctrl-0 = <&uart2_xfer>;
			status = "okay";
		};
	};
};
