/*
 * Copyright 2013 Freescale Semiconductor, Inc.
 *
 * Author: Fabio Estevam <fabio.estevam@freescale.com>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 *
 */

/ {
	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_2p5v: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "2P5V";
			regulator-min-microvolt = <2500000>;
			regulator-max-microvolt = <2500000>;
			regulator-always-on;
		};

		reg_3p3v: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "3P3V";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};
	};

	sound {
		compatible = "fsl,imx6-wandboard-sgtl5000",
			     "fsl,imx-audio-sgtl5000";
		model = "imx6-wandboard-sgtl5000";
		ssi-controller = <&ssi1>;
		audio-codec = <&codec>;
		audio-routing =
			"MIC_IN", "Mic Jack",
			"Mic Jack", "Mic Bias",
			"Headphone Jack", "HP_OUT";
		mux-int-port = <1>;
		mux-ext-port = <3>;
	};

	sound-spdif {
		compatible = "fsl,imx-audio-spdif";
		model = "imx-spdif";
		spdif-controller = <&spdif>;
		spdif-out;
	};
};

&audmux {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_audmux>;
	status = "okay";
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	codec: sgtl5000@0a {
		compatible = "fsl,sgtl5000";
		reg = <0x0a>;
		clocks = <&clks 201>;
		VDDA-supply = <&reg_2p5v>;
		VDDIO-supply = <&reg_3p3v>;
	};
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	imx6qdl-wandboard {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				MX6QDL_PAD_GPIO_0__CCM_CLKO1 	 0x130b0
				MX6QDL_PAD_GPIO_2__GPIO1_IO02	 0x80000000
				MX6QDL_PAD_EIM_DA9__GPIO3_IO09	 0x80000000
				MX6QDL_PAD_EIM_EB1__GPIO2_IO29   0x80000000 /* WL_REF_ON */
				MX6QDL_PAD_EIM_A25__GPIO5_IO02   0x80000000 /* WL_RST_N */
				MX6QDL_PAD_ENET_RXD1__GPIO1_IO26 0x80000000 /* WL_REG_ON */
				MX6QDL_PAD_ENET_TXD1__GPIO1_IO29 0x80000000 /* WL_HOST_WAKE */
				MX6QDL_PAD_ENET_TXD0__GPIO1_IO30 0x80000000 /* WL_WAKE */
				MX6QDL_PAD_EIM_D29__GPIO3_IO29   0x80000000
			>;
		};

		pinctrl_audmux: audmuxgrp {
			fsl,pins = <
				MX6QDL_PAD_CSI0_DAT7__AUD3_RXD		0x130b0
				MX6QDL_PAD_CSI0_DAT4__AUD3_TXC		0x130b0
				MX6QDL_PAD_CSI0_DAT5__AUD3_TXD		0x110b0
				MX6QDL_PAD_CSI0_DAT6__AUD3_TXFS		0x130b0
			>;
		};

		pinctrl_enet: enetgrp {
			fsl,pins = <
				MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b0b0
				MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
				MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b0b0
				MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b0b0
				MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b0b0
				MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b0b0
				MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b0b0
				MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b0b0
				MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x1b0b0
				MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b0b0
				MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x1b0b0
				MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x1b0b0
				MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b0b0
				MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b0b0
				MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x1b0b0
				MX6QDL_PAD_GPIO_16__ENET_REF_CLK	0x4001b0a8
				MX6QDL_PAD_GPIO_6__ENET_IRQ		0x000b1
			>;
		};

		pinctrl_i2c2: i2c2grp {
			fsl,pins = <
				MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b8b1
				MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b8b1
			>;
		};

		pinctrl_spdif: spdifgrp {
			fsl,pins = <
				MX6QDL_PAD_ENET_RXD0__SPDIF_OUT		0x1b0b0
			>;
		};

		pinctrl_uart1: uart1grp {
			fsl,pins = <
				MX6QDL_PAD_CSI0_DAT10__UART1_TX_DATA	0x1b0b1
				MX6QDL_PAD_CSI0_DAT11__UART1_RX_DATA	0x1b0b1
			>;
		};

		pinctrl_uart3: uart3grp {
			fsl,pins = <
				MX6QDL_PAD_EIM_D24__UART3_TX_DATA	0x1b0b1
				MX6QDL_PAD_EIM_D25__UART3_RX_DATA	0x1b0b1
				MX6QDL_PAD_EIM_D23__UART3_CTS_B		0x1b0b1
				MX6QDL_PAD_EIM_EB3__UART3_RTS_B		0x1b0b1
			>;
		};

		pinctrl_usbotg: usbotggrp {
			fsl,pins = <
				MX6QDL_PAD_GPIO_1__USB_OTG_ID		0x17059
			>;
		};

		pinctrl_usdhc1: usdhc1grp {
			fsl,pins = <
				MX6QDL_PAD_SD1_CMD__SD1_CMD		0x17059
				MX6QDL_PAD_SD1_CLK__SD1_CLK		0x10059
				MX6QDL_PAD_SD1_DAT0__SD1_DATA0		0x17059
				MX6QDL_PAD_SD1_DAT1__SD1_DATA1		0x17059
				MX6QDL_PAD_SD1_DAT2__SD1_DATA2		0x17059
				MX6QDL_PAD_SD1_DAT3__SD1_DATA3		0x17059
			>;
		};

		pinctrl_usdhc2: usdhc2grp {
			fsl,pins = <
				MX6QDL_PAD_SD2_CMD__SD2_CMD		0x17059
				MX6QDL_PAD_SD2_CLK__SD2_CLK		0x10059
				MX6QDL_PAD_SD2_DAT0__SD2_DATA0		0x17059
				MX6QDL_PAD_SD2_DAT1__SD2_DATA1		0x17059
				MX6QDL_PAD_SD2_DAT2__SD2_DATA2		0x17059
				MX6QDL_PAD_SD2_DAT3__SD2_DATA3		0x17059
			>;
		};

		pinctrl_usdhc3: usdhc3grp {
			fsl,pins = <
				MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17059
				MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10059
				MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17059
				MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17059
				MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17059
				MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17059
			>;
		};
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	phy-reset-gpios = <&gpio3 29 0>;
	interrupts-extended = <&gpio1 6 IRQ_TYPE_LEVEL_HIGH>,
			      <&intc 0 119 IRQ_TYPE_LEVEL_HIGH>;
	status = "okay";
};

&spdif {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_spdif>;
	status = "okay";
};

&ssi1 {
	fsl,mode = "i2s-slave";
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	fsl,uart-has-rtscts;
	status = "okay";
};

&usbh1 {
	status = "okay";
};

&usbotg {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	disable-over-current;
	dr_mode = "peripheral";
	status = "okay";
};

&usdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc1>;
	cd-gpios = <&gpio1 2 0>;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2>;
	non-removable;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	cd-gpios = <&gpio3 9 0>;
	status = "okay";
};
