/*
 * Copyright 2014 Open Source Support GmbH
 *
 * David Lanzendörfer <david.lanzendoerfer@o2s.ch>
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
/include/ "sun4i-a10.dtsi"
/include/ "sunxi-common-regulators.dtsi"

/ {
	model = "INet-97F Rev 02";
	compatible = "primux,inet97fv2", "allwinner,sun4i-a10";

	aliases {
		serial0 = &uart0;
	};

	soc@01c00000 {
		uart0: serial@01c28000 {
			pinctrl-names = "default";
			pinctrl-0 = <&uart0_pins_a>;
			status = "okay";
		};

		i2c0: i2c@01c2ac00 {
			pinctrl-names = "default";
			pinctrl-0 = <&i2c0_pins_a>;
			status = "okay";
		};

		usbphy: phy@01c13400 {
			usb1_vbus-supply = <&reg_usb1_vbus>;
			usb2_vbus-supply = <&reg_usb2_vbus>;
			status = "okay";
		};

		ehci0: usb@01c14000 {
			status = "okay";
		};

		ohci0: usb@01c14400 {
			status = "okay";
		};

		ehci1: usb@01c1c000 {
			status = "okay";
		};

		ohci1: usb@01c1c400 {
			status = "okay";
		};
	};

	reg_usb1_vbus: usb1-vbus {
		status = "okay";
	};

	reg_usb2_vbus: usb2-vbus {
		status = "okay";
	};
};
