/*
 * Copyright (C) 2013 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/dts-v1/;

#include "omap2430.dtsi"

/ {
	model = "TI OMAP2430 SDP";
	compatible = "ti,omap2430-sdp", "ti,omap2430", "ti,omap2";

	memory {
		device_type = "memory";
		reg = <0x80000000 0x8000000>; /* 128 MB */
	};
};

&i2c2 {
	clock-frequency = <100000>;

	twl: twl@48 {
		reg = <0x48>;
		interrupts = <7>; /* SYS_NIRQ cascaded to intc */
	};
};

#include "twl4030.dtsi"

&mmc1 {
	vmmc-supply = <&vmmc1>;
	bus-width = <4>;
};

&gpmc {
	ranges = <5 0 0x08000000 0x01000000>;
	ethernet@gpmc {
		compatible = "smsc,lan91c94";
		interrupt-parent = <&gpio5>;
		interrupts = <21 IRQ_TYPE_LEVEL_LOW>;	/* gpio149 */
		reg = <5 0x300 0xf>;
		bank-width = <2>;
		gpmc,mux-add-data;
        };
};

