/*
 * Device Tree Source for am3517 SoC
 *
 * Copyright (C) 2013 Texas Instruments Incorporated - http://www.ti.com/
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

#include "omap3.dtsi"

/ {
	aliases {
		serial3 = &uart4;
	};

	ocp {
		am35x_otg_hs: am35x_otg_hs@5c040000 {
			compatible = "ti,omap3-musb";
			ti,hwmods = "am35x_otg_hs";
			status = "disabled";
			reg = <0x5c040000 0x1000>;
			interrupts = <71>;
			interrupt-names = "mc";
		};

		davinci_emac: ethernet@0x5c000000 {
			compatible = "ti,am3517-emac";
			ti,hwmods = "davinci_emac";
			status = "disabled";
			reg = <0x5c000000 0x30000>;
			interrupts = <67 68 69 70>;
			ti,davinci-ctrl-reg-offset = <0x10000>;
			ti,davinci-ctrl-mod-reg-offset = <0>;
			ti,davinci-ctrl-ram-offset = <0x20000>;
			ti,davinci-ctrl-ram-size = <0x2000>;
			ti,davinci-rmii-en = /bits/ 8 <1>;
			local-mac-address = [ 00 00 00 00 00 00 ];
		};

		davinci_mdio: ethernet@0x5c030000 {
			compatible = "ti,davinci_mdio";
			ti,hwmods = "davinci_mdio";
			status = "disabled";
			reg = <0x5c030000 0x1000>;
			bus_freq = <1000000>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		uart4: serial@4809e000 {
			compatible = "ti,omap3-uart";
			ti,hwmods = "uart4";
			status = "disabled";
			reg = <0x4809e000 0x400>;
			interrupts = <84>;
			dmas = <&sdma 55 &sdma 54>;
			dma-names = "tx", "rx";
			clock-frequency = <48000000>;
		};
	};
};

/include/ "am35xx-clocks.dtsi"
/include/ "omap36xx-am35xx-omap3430es2plus-clocks.dtsi"
