/*
 * Copyright 2012 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;

#include "imx6q.dtsi"
#include "imx6qdl-sabresd.dtsi"

/ {
	model = "Freescale i.MX6 Quad SABRE Smart Device Board";
	compatible = "fsl,imx6q-sabresd", "fsl,imx6q";

	chosen {
		linux,stdout-path = "/soc/aips-bus@02000000/spba-bus@02000000/serial@02020000";
	};
};

&iomuxc {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_hog>;

	hog {
		pinctrl_hog: hoggrp {
			fsl,pins = <
				MX6Q_PAD_GPIO_4__GPIO1_IO04   0x80000000
				MX6Q_PAD_GPIO_5__GPIO1_IO05   0x80000000
				MX6Q_PAD_NANDF_D0__GPIO2_IO00 0x80000000
				MX6Q_PAD_NANDF_D1__GPIO2_IO01 0x80000000
				MX6Q_PAD_NANDF_D2__GPIO2_IO02 0x80000000
				MX6Q_PAD_NANDF_D3__GPIO2_IO03 0x80000000
			>;
		};
	};
};
