/*
 * Copyright 2012 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/ {
	memory {
		reg = <0x10000000 0x40000000>;
	};

	regulators {
		compatible = "simple-bus";

		reg_usb_otg_vbus: usb_otg_vbus {
			compatible = "regulator-fixed";
			regulator-name = "usb_otg_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			gpio = <&gpio3 22 0>;
			enable-active-high;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		volume-up {
			label = "Volume Up";
			gpios = <&gpio1 4 0>;
			linux,code = <115>; /* KEY_VOLUMEUP */
		};

		volume-down {
			label = "Volume Down";
			gpios = <&gpio1 5 0>;
			linux,code = <114>; /* KEY_VOLUMEDOWN */
		};
	};
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet_1>;
	phy-mode = "rgmii";
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1_1>;
	status = "okay";
};

&usbh1 {
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_usb_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg_2>;
	disable-over-current;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2_1>;
	cd-gpios = <&gpio2 2 0>;
	wp-gpios = <&gpio2 3 0>;
	status = "okay";
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3_1>;
	cd-gpios = <&gpio2 0 0>;
	wp-gpios = <&gpio2 1 0>;
	status = "okay";
};
