/*
 * Copyright 2011 Freescale Semiconductor, Inc.
 * Copyright 2011 Linaro Ltd.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

#include "skeleton.dtsi"

/ {
	aliases {
		serial0 = &uart1;
		serial1 = &uart2;
		serial2 = &uart3;
		serial3 = &uart4;
		serial4 = &uart5;
		gpio0 = &gpio1;
		gpio1 = &gpio2;
		gpio2 = &gpio3;
		gpio3 = &gpio4;
		gpio4 = &gpio5;
		gpio5 = &gpio6;
		gpio6 = &gpio7;
		mmc0 = &usdhc1;
		mmc1 = &usdhc2;
		mmc2 = &usdhc3;
		mmc3 = &usdhc4;
	};

	intc: interrupt-controller@00a01000 {
		compatible = "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		#address-cells = <1>;
		#size-cells = <1>;
		interrupt-controller;
		reg = <0x00a01000 0x1000>,
		      <0x00a00100 0x100>;
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <0>;

		ckil {
			compatible = "fsl,imx-ckil", "fixed-clock";
			clock-frequency = <32768>;
		};

		ckih1 {
			compatible = "fsl,imx-ckih1", "fixed-clock";
			clock-frequency = <0>;
		};

		osc {
			compatible = "fsl,imx-osc", "fixed-clock";
			clock-frequency = <24000000>;
		};
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		interrupt-parent = <&intc>;
		ranges;

		dma_apbh: dma-apbh@00110000 {
			compatible = "fsl,imx6q-dma-apbh", "fsl,imx28-dma-apbh";
			reg = <0x00110000 0x2000>;
			interrupts = <0 13 0x04>, <0 13 0x04>, <0 13 0x04>, <0 13 0x04>;
			interrupt-names = "gpmi0", "gpmi1", "gpmi2", "gpmi3";
			#dma-cells = <1>;
			dma-channels = <4>;
			clocks = <&clks 106>;
		};

		gpmi: gpmi-nand@00112000 {
			compatible = "fsl,imx6q-gpmi-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x00112000 0x2000>, <0x00114000 0x2000>;
			reg-names = "gpmi-nand", "bch";
			interrupts = <0 13 0x04>, <0 15 0x04>;
			interrupt-names = "gpmi-dma", "bch";
			clocks = <&clks 152>, <&clks 153>, <&clks 151>,
				 <&clks 150>, <&clks 149>;
			clock-names = "gpmi_io", "gpmi_apb", "gpmi_bch",
				      "gpmi_bch_apb", "per1_bch";
			dmas = <&dma_apbh 0>;
			dma-names = "rx-tx";
			fsl,gpmi-dma-channel = <0>;
			status = "disabled";
		};

		timer@00a00600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0x00a00600 0x20>;
			interrupts = <1 13 0xf01>;
			clocks = <&clks 15>;
		};

		L2: l2-cache@00a02000 {
			compatible = "arm,pl310-cache";
			reg = <0x00a02000 0x1000>;
			interrupts = <0 92 0x04>;
			cache-unified;
			cache-level = <2>;
		};

		pmu {
			compatible = "arm,cortex-a9-pmu";
			interrupts = <0 94 0x04>;
		};

		aips-bus@02000000 { /* AIPS1 */
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02000000 0x100000>;
			ranges;

			spba-bus@02000000 {
				compatible = "fsl,spba-bus", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0x02000000 0x40000>;
				ranges;

				spdif: spdif@02004000 {
					reg = <0x02004000 0x4000>;
					interrupts = <0 52 0x04>;
				};

				ecspi1: ecspi@02008000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6q-ecspi", "fsl,imx51-ecspi";
					reg = <0x02008000 0x4000>;
					interrupts = <0 31 0x04>;
					clocks = <&clks 112>, <&clks 112>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi2: ecspi@0200c000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6q-ecspi", "fsl,imx51-ecspi";
					reg = <0x0200c000 0x4000>;
					interrupts = <0 32 0x04>;
					clocks = <&clks 113>, <&clks 113>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi3: ecspi@02010000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6q-ecspi", "fsl,imx51-ecspi";
					reg = <0x02010000 0x4000>;
					interrupts = <0 33 0x04>;
					clocks = <&clks 114>, <&clks 114>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				ecspi4: ecspi@02014000 {
					#address-cells = <1>;
					#size-cells = <0>;
					compatible = "fsl,imx6q-ecspi", "fsl,imx51-ecspi";
					reg = <0x02014000 0x4000>;
					interrupts = <0 34 0x04>;
					clocks = <&clks 115>, <&clks 115>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				uart1: serial@02020000 {
					compatible = "fsl,imx6q-uart", "fsl,imx21-uart";
					reg = <0x02020000 0x4000>;
					interrupts = <0 26 0x04>;
					clocks = <&clks 160>, <&clks 161>;
					clock-names = "ipg", "per";
					status = "disabled";
				};

				esai: esai@02024000 {
					reg = <0x02024000 0x4000>;
					interrupts = <0 51 0x04>;
				};

				ssi1: ssi@02028000 {
					compatible = "fsl,imx6q-ssi","fsl,imx21-ssi";
					reg = <0x02028000 0x4000>;
					interrupts = <0 46 0x04>;
					clocks = <&clks 178>;
					fsl,fifo-depth = <15>;
					fsl,ssi-dma-events = <38 37>;
					status = "disabled";
				};

				ssi2: ssi@0202c000 {
					compatible = "fsl,imx6q-ssi","fsl,imx21-ssi";
					reg = <0x0202c000 0x4000>;
					interrupts = <0 47 0x04>;
					clocks = <&clks 179>;
					fsl,fifo-depth = <15>;
					fsl,ssi-dma-events = <42 41>;
					status = "disabled";
				};

				ssi3: ssi@02030000 {
					compatible = "fsl,imx6q-ssi","fsl,imx21-ssi";
					reg = <0x02030000 0x4000>;
					interrupts = <0 48 0x04>;
					clocks = <&clks 180>;
					fsl,fifo-depth = <15>;
					fsl,ssi-dma-events = <46 45>;
					status = "disabled";
				};

				asrc: asrc@02034000 {
					reg = <0x02034000 0x4000>;
					interrupts = <0 50 0x04>;
				};

				spba@0203c000 {
					reg = <0x0203c000 0x4000>;
				};
			};

			vpu: vpu@02040000 {
				reg = <0x02040000 0x3c000>;
				interrupts = <0 3 0x04 0 12 0x04>;
			};

			aipstz@0207c000 { /* AIPSTZ1 */
				reg = <0x0207c000 0x4000>;
			};

			pwm1: pwm@02080000 {
				#pwm-cells = <2>;
				compatible = "fsl,imx6q-pwm", "fsl,imx27-pwm";
				reg = <0x02080000 0x4000>;
				interrupts = <0 83 0x04>;
				clocks = <&clks 62>, <&clks 145>;
				clock-names = "ipg", "per";
			};

			pwm2: pwm@02084000 {
				#pwm-cells = <2>;
				compatible = "fsl,imx6q-pwm", "fsl,imx27-pwm";
				reg = <0x02084000 0x4000>;
				interrupts = <0 84 0x04>;
				clocks = <&clks 62>, <&clks 146>;
				clock-names = "ipg", "per";
			};

			pwm3: pwm@02088000 {
				#pwm-cells = <2>;
				compatible = "fsl,imx6q-pwm", "fsl,imx27-pwm";
				reg = <0x02088000 0x4000>;
				interrupts = <0 85 0x04>;
				clocks = <&clks 62>, <&clks 147>;
				clock-names = "ipg", "per";
			};

			pwm4: pwm@0208c000 {
				#pwm-cells = <2>;
				compatible = "fsl,imx6q-pwm", "fsl,imx27-pwm";
				reg = <0x0208c000 0x4000>;
				interrupts = <0 86 0x04>;
				clocks = <&clks 62>, <&clks 148>;
				clock-names = "ipg", "per";
			};

			can1: flexcan@02090000 {
				reg = <0x02090000 0x4000>;
				interrupts = <0 110 0x04>;
			};

			can2: flexcan@02094000 {
				reg = <0x02094000 0x4000>;
				interrupts = <0 111 0x04>;
			};

			gpt: gpt@02098000 {
				compatible = "fsl,imx6q-gpt", "fsl,imx31-gpt";
				reg = <0x02098000 0x4000>;
				interrupts = <0 55 0x04>;
				clocks = <&clks 119>, <&clks 120>;
				clock-names = "ipg", "per";
			};

			gpio1: gpio@0209c000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x0209c000 0x4000>;
				interrupts = <0 66 0x04 0 67 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio2: gpio@020a0000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020a0000 0x4000>;
				interrupts = <0 68 0x04 0 69 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio3: gpio@020a4000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020a4000 0x4000>;
				interrupts = <0 70 0x04 0 71 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio4: gpio@020a8000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020a8000 0x4000>;
				interrupts = <0 72 0x04 0 73 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio5: gpio@020ac000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020ac000 0x4000>;
				interrupts = <0 74 0x04 0 75 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio6: gpio@020b0000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020b0000 0x4000>;
				interrupts = <0 76 0x04 0 77 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			gpio7: gpio@020b4000 {
				compatible = "fsl,imx6q-gpio", "fsl,imx35-gpio";
				reg = <0x020b4000 0x4000>;
				interrupts = <0 78 0x04 0 79 0x04>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};

			kpp: kpp@020b8000 {
				reg = <0x020b8000 0x4000>;
				interrupts = <0 82 0x04>;
			};

			wdog1: wdog@020bc000 {
				compatible = "fsl,imx6q-wdt", "fsl,imx21-wdt";
				reg = <0x020bc000 0x4000>;
				interrupts = <0 80 0x04>;
				clocks = <&clks 0>;
			};

			wdog2: wdog@020c0000 {
				compatible = "fsl,imx6q-wdt", "fsl,imx21-wdt";
				reg = <0x020c0000 0x4000>;
				interrupts = <0 81 0x04>;
				clocks = <&clks 0>;
				status = "disabled";
			};

			clks: ccm@020c4000 {
				compatible = "fsl,imx6q-ccm";
				reg = <0x020c4000 0x4000>;
				interrupts = <0 87 0x04 0 88 0x04>;
				#clock-cells = <1>;
			};

			anatop: anatop@020c8000 {
				compatible = "fsl,imx6q-anatop", "syscon", "simple-bus";
				reg = <0x020c8000 0x1000>;
				interrupts = <0 49 0x04 0 54 0x04 0 127 0x04>;

				regulator-1p1@110 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd1p1";
					regulator-min-microvolt = <800000>;
					regulator-max-microvolt = <1375000>;
					regulator-always-on;
					anatop-reg-offset = <0x110>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <4>;
					anatop-min-voltage = <800000>;
					anatop-max-voltage = <1375000>;
				};

				regulator-3p0@120 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd3p0";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <3150000>;
					regulator-always-on;
					anatop-reg-offset = <0x120>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2625000>;
					anatop-max-voltage = <3400000>;
				};

				regulator-2p5@130 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vdd2p5";
					regulator-min-microvolt = <2000000>;
					regulator-max-microvolt = <2750000>;
					regulator-always-on;
					anatop-reg-offset = <0x130>;
					anatop-vol-bit-shift = <8>;
					anatop-vol-bit-width = <5>;
					anatop-min-bit-val = <0>;
					anatop-min-voltage = <2000000>;
					anatop-max-voltage = <2750000>;
				};

				reg_arm: regulator-vddcore@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "cpu";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <0>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <24>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_pu: regulator-vddpu@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddpu";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <9>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <26>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};

				reg_soc: regulator-vddsoc@140 {
					compatible = "fsl,anatop-regulator";
					regulator-name = "vddsoc";
					regulator-min-microvolt = <725000>;
					regulator-max-microvolt = <1450000>;
					regulator-always-on;
					anatop-reg-offset = <0x140>;
					anatop-vol-bit-shift = <18>;
					anatop-vol-bit-width = <5>;
					anatop-delay-reg-offset = <0x170>;
					anatop-delay-bit-shift = <28>;
					anatop-delay-bit-width = <2>;
					anatop-min-bit-val = <1>;
					anatop-min-voltage = <725000>;
					anatop-max-voltage = <1450000>;
				};
			};

			usbphy1: usbphy@020c9000 {
				compatible = "fsl,imx6q-usbphy", "fsl,imx23-usbphy";
				reg = <0x020c9000 0x1000>;
				interrupts = <0 44 0x04>;
				clocks = <&clks 182>;
			};

			usbphy2: usbphy@020ca000 {
				compatible = "fsl,imx6q-usbphy", "fsl,imx23-usbphy";
				reg = <0x020ca000 0x1000>;
				interrupts = <0 45 0x04>;
				clocks = <&clks 183>;
			};

			snvs@020cc000 {
				compatible = "fsl,sec-v4.0-mon", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x020cc000 0x4000>;

				snvs-rtc-lp@34 {
					compatible = "fsl,sec-v4.0-mon-rtc-lp";
					reg = <0x34 0x58>;
					interrupts = <0 19 0x04 0 20 0x04>;
				};
			};

			epit1: epit@020d0000 { /* EPIT1 */
				reg = <0x020d0000 0x4000>;
				interrupts = <0 56 0x04>;
			};

			epit2: epit@020d4000 { /* EPIT2 */
				reg = <0x020d4000 0x4000>;
				interrupts = <0 57 0x04>;
			};

			src: src@020d8000 {
				compatible = "fsl,imx6q-src", "fsl,imx51-src";
				reg = <0x020d8000 0x4000>;
				interrupts = <0 91 0x04 0 96 0x04>;
				#reset-cells = <1>;
			};

			gpc: gpc@020dc000 {
				compatible = "fsl,imx6q-gpc";
				reg = <0x020dc000 0x4000>;
				interrupts = <0 89 0x04 0 90 0x04>;
			};

			gpr: iomuxc-gpr@020e0000 {
				compatible = "fsl,imx6q-iomuxc-gpr", "syscon";
				reg = <0x020e0000 0x38>;
			};

			ldb: ldb@020e0008 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6q-ldb", "fsl,imx53-ldb";
				gpr = <&gpr>;
				status = "disabled";

				lvds-channel@0 {
					reg = <0>;
					crtcs = <&ipu1 0>;
					status = "disabled";
				};

				lvds-channel@1 {
					reg = <1>;
					crtcs = <&ipu1 1>;
					status = "disabled";
				};
			};

			dcic1: dcic@020e4000 {
				reg = <0x020e4000 0x4000>;
				interrupts = <0 124 0x04>;
			};

			dcic2: dcic@020e8000 {
				reg = <0x020e8000 0x4000>;
				interrupts = <0 125 0x04>;
			};

			sdma: sdma@020ec000 {
				compatible = "fsl,imx6q-sdma", "fsl,imx35-sdma";
				reg = <0x020ec000 0x4000>;
				interrupts = <0 2 0x04>;
				clocks = <&clks 155>, <&clks 155>;
				clock-names = "ipg", "ahb";
				fsl,sdma-ram-script-name = "imx/sdma/sdma-imx6q.bin";
			};
		};

		aips-bus@02100000 { /* AIPS2 */
			compatible = "fsl,aips-bus", "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x02100000 0x100000>;
			ranges;

			caam@02100000 {
				reg = <0x02100000 0x40000>;
				interrupts = <0 105 0x04 0 106 0x04>;
			};

			aipstz@0217c000 { /* AIPSTZ2 */
				reg = <0x0217c000 0x4000>;
			};

			usbotg: usb@02184000 {
				compatible = "fsl,imx6q-usb", "fsl,imx27-usb";
				reg = <0x02184000 0x200>;
				interrupts = <0 43 0x04>;
				clocks = <&clks 162>;
				fsl,usbphy = <&usbphy1>;
				fsl,usbmisc = <&usbmisc 0>;
				status = "disabled";
			};

			usbh1: usb@02184200 {
				compatible = "fsl,imx6q-usb", "fsl,imx27-usb";
				reg = <0x02184200 0x200>;
				interrupts = <0 40 0x04>;
				clocks = <&clks 162>;
				fsl,usbphy = <&usbphy2>;
				fsl,usbmisc = <&usbmisc 1>;
				status = "disabled";
			};

			usbh2: usb@02184400 {
				compatible = "fsl,imx6q-usb", "fsl,imx27-usb";
				reg = <0x02184400 0x200>;
				interrupts = <0 41 0x04>;
				clocks = <&clks 162>;
				fsl,usbmisc = <&usbmisc 2>;
				status = "disabled";
			};

			usbh3: usb@02184600 {
				compatible = "fsl,imx6q-usb", "fsl,imx27-usb";
				reg = <0x02184600 0x200>;
				interrupts = <0 42 0x04>;
				clocks = <&clks 162>;
				fsl,usbmisc = <&usbmisc 3>;
				status = "disabled";
			};

			usbmisc: usbmisc@02184800 {
				#index-cells = <1>;
				compatible = "fsl,imx6q-usbmisc";
				reg = <0x02184800 0x200>;
				clocks = <&clks 162>;
			};

			fec: ethernet@02188000 {
				compatible = "fsl,imx6q-fec";
				reg = <0x02188000 0x4000>;
				interrupts = <0 118 0x04 0 119 0x04>;
				clocks = <&clks 117>, <&clks 117>, <&clks 190>;
				clock-names = "ipg", "ahb", "ptp";
				status = "disabled";
			};

			mlb@0218c000 {
				reg = <0x0218c000 0x4000>;
				interrupts = <0 53 0x04 0 117 0x04 0 126 0x04>;
			};

			usdhc1: usdhc@02190000 {
				compatible = "fsl,imx6q-usdhc";
				reg = <0x02190000 0x4000>;
				interrupts = <0 22 0x04>;
				clocks = <&clks 163>, <&clks 163>, <&clks 163>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc2: usdhc@02194000 {
				compatible = "fsl,imx6q-usdhc";
				reg = <0x02194000 0x4000>;
				interrupts = <0 23 0x04>;
				clocks = <&clks 164>, <&clks 164>, <&clks 164>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc3: usdhc@02198000 {
				compatible = "fsl,imx6q-usdhc";
				reg = <0x02198000 0x4000>;
				interrupts = <0 24 0x04>;
				clocks = <&clks 165>, <&clks 165>, <&clks 165>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			usdhc4: usdhc@0219c000 {
				compatible = "fsl,imx6q-usdhc";
				reg = <0x0219c000 0x4000>;
				interrupts = <0 25 0x04>;
				clocks = <&clks 166>, <&clks 166>, <&clks 166>;
				clock-names = "ipg", "ahb", "per";
				bus-width = <4>;
				status = "disabled";
			};

			i2c1: i2c@021a0000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6q-i2c", "fsl,imx21-i2c";
				reg = <0x021a0000 0x4000>;
				interrupts = <0 36 0x04>;
				clocks = <&clks 125>;
				status = "disabled";
			};

			i2c2: i2c@021a4000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6q-i2c", "fsl,imx21-i2c";
				reg = <0x021a4000 0x4000>;
				interrupts = <0 37 0x04>;
				clocks = <&clks 126>;
				status = "disabled";
			};

			i2c3: i2c@021a8000 {
				#address-cells = <1>;
				#size-cells = <0>;
				compatible = "fsl,imx6q-i2c", "fsl,imx21-i2c";
				reg = <0x021a8000 0x4000>;
				interrupts = <0 38 0x04>;
				clocks = <&clks 127>;
				status = "disabled";
			};

			romcp@021ac000 {
				reg = <0x021ac000 0x4000>;
			};

			mmdc0: mmdc@021b0000 { /* MMDC0 */
				compatible = "fsl,imx6q-mmdc";
				reg = <0x021b0000 0x4000>;
			};

			mmdc1: mmdc@021b4000 { /* MMDC1 */
				reg = <0x021b4000 0x4000>;
			};

			weim@021b8000 {
				reg = <0x021b8000 0x4000>;
				interrupts = <0 14 0x04>;
			};

			ocotp@021bc000 {
				compatible = "fsl,imx6q-ocotp";
				reg = <0x021bc000 0x4000>;
			};

			ocotp@021c0000 {
				reg = <0x021c0000 0x4000>;
				interrupts = <0 21 0x04>;
			};

			tzasc@021d0000 { /* TZASC1 */
				reg = <0x021d0000 0x4000>;
				interrupts = <0 108 0x04>;
			};

			tzasc@021d4000 { /* TZASC2 */
				reg = <0x021d4000 0x4000>;
				interrupts = <0 109 0x04>;
			};

			audmux: audmux@021d8000 {
				compatible = "fsl,imx6q-audmux", "fsl,imx31-audmux";
				reg = <0x021d8000 0x4000>;
				status = "disabled";
			};

			mipi@021dc000 { /* MIPI-CSI */
				reg = <0x021dc000 0x4000>;
			};

			mipi@021e0000 { /* MIPI-DSI */
				reg = <0x021e0000 0x4000>;
			};

			vdoa@021e4000 {
				reg = <0x021e4000 0x4000>;
				interrupts = <0 18 0x04>;
			};

			uart2: serial@021e8000 {
				compatible = "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021e8000 0x4000>;
				interrupts = <0 27 0x04>;
				clocks = <&clks 160>, <&clks 161>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart3: serial@021ec000 {
				compatible = "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021ec000 0x4000>;
				interrupts = <0 28 0x04>;
				clocks = <&clks 160>, <&clks 161>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart4: serial@021f0000 {
				compatible = "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021f0000 0x4000>;
				interrupts = <0 29 0x04>;
				clocks = <&clks 160>, <&clks 161>;
				clock-names = "ipg", "per";
				status = "disabled";
			};

			uart5: serial@021f4000 {
				compatible = "fsl,imx6q-uart", "fsl,imx21-uart";
				reg = <0x021f4000 0x4000>;
				interrupts = <0 30 0x04>;
				clocks = <&clks 160>, <&clks 161>;
				clock-names = "ipg", "per";
				status = "disabled";
			};
		};

		sata: sata@02200000 {
			compatible = "fsl,imx6q-ahci";
			reg = <0x02200000 0x4000>;
			interrupts = <0 39 0x04>;
			clocks = <&clks 154 &clks 105 &clks 187>;
			clock-names = "ipg", "ahb", "per";
			gprreg = <&gpr>;
			status = "disabled";
		};

		ipu1: ipu@02400000 {
			#crtc-cells = <1>;
			compatible = "fsl,imx6q-ipu";
			reg = <0x02400000 0x400000>;
			interrupts = <0 6 0x4 0 5 0x4>;
			clocks = <&clks 130>, <&clks 131>, <&clks 132>;
			clock-names = "bus", "di0", "di1";
			resets = <&src 2>;
		};
	};
};
