/* s-record file with linear addresses for MicroBoot/OpenBLT */
OPENFILE "%ABS_FILE%.sx"
format = motorola
busWidth = 1
len = 0x4000

/* logical non banked flash at $4000 and $C000 to physical */
origin = 0x004000
destination = 0x34000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x00C000
destination = 0x3C000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

/* logical 128 kB banked flash to physical */
origin = 0x088000
destination = 0x020000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x098000
destination = 0x024000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0A8000
destination = 0x028000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0B8000
destination = 0x02C000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0C8000
destination = 0x030000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0D8000
destination = 0x034000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0E8000
destination = 0x038000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

origin = 0x0F8000
destination = 0x03C000
len = 0x4000
SENDBYTE 1 "%ABS_FILE%"

CLOSE

