From 2613f95f614b39681f77a5036046ea395e306e28 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Fri, 6 Dec 2013 13:01:31 -0800
Subject: [PATCH] net: phy: use phy_init_hw instead of open-coding it

Use phy_init_hw() instead of open-coding it in phy_mii_ioctl(), this
improves consistenty and makes sure that we will not duplicate the same
routine somewhere else.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/phy.c | 7 ++-----
 1 file changed, 2 insertions(+), 5 deletions(-)

diff --git a/drivers/net/phy/phy.c b/drivers/net/phy/phy.c
index 05cb8fe..5d7101b 100644
--- a/drivers/net/phy/phy.c
+++ b/drivers/net/phy/phy.c
@@ -361,11 +361,8 @@ int phy_mii_ioctl(struct phy_device *phydev,
 			      mii_data->reg_num, val);
 
 		if (mii_data->reg_num == MII_BMCR &&
-		    val & BMCR_RESET &&
-		    phydev->drv->config_init) {
-			phy_scan_fixups(phydev);
-			phydev->drv->config_init(phydev);
-		}
+		    val & BMCR_RESET)
+			phy_init_hw(phydev);
 		break;
 
 	case SIOCSHWTSTAMP:
-- 
2.3.5

