From 9bea8b61f6025cd633bd5ac71be258620b49bcb3 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 2 Sep 2013 11:00:06 +0200
Subject: [PATCH] rt2x00: rt2800lib: fix max supported beacon count for RT3593

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/rt2x00/rt2800lib.c |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/rt2x00/rt2800lib.c
@@ -7864,7 +7864,10 @@ int rt2800_probe_hw(struct rt2x00_dev *r
 	if (rt2x00_rt(rt2x00dev, RT3593))
 		__set_bit(RT2800_HAS_HIGH_SHARED_MEM, &drv_data->rt2800_flags);
 
-	drv_data->hw_beacon_count = 8;
+	if (rt2x00_rt(rt2x00dev, RT3593))
+		drv_data->hw_beacon_count = 16;
+	else
+		drv_data->hw_beacon_count = 8;
 
 	/*
 	 * Allocate eeprom data.
