From c76bf0b3b33a00eb7a8bd274a84d3b0cae93a5b9 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dsteve@broadcom.com>
Date: Mon, 9 Dec 2013 11:01:53 +0000
Subject: [PATCH 132/174] V4L2: Correct JPEG Q-factor range

Should be 1-100, not 0-100

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>
---
 drivers/media/platform/bcm2835/controls.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/media/platform/bcm2835/controls.c
+++ b/drivers/media/platform/bcm2835/controls.c
@@ -538,7 +538,7 @@ static int ctrl_set_bitrate_mode(struct
 	return 0;
 }
 
-static int ctrl_set_q_factor(struct bm2835_mmal_dev *dev,
+static int ctrl_set_image_encode_output(struct bm2835_mmal_dev *dev,
 		      struct v4l2_ctrl *ctrl,
 		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
 {
@@ -683,9 +683,9 @@ static const struct bm2835_mmal_v4l2_ctr
 	},
 	{
 		V4L2_CID_JPEG_COMPRESSION_QUALITY, MMAL_CONTROL_TYPE_STD,
-		0, 100,
+		1, 100,
 		30, 1, NULL,
-		MMAL_PARAMETER_JPEG_Q_FACTOR, &ctrl_set_q_factor
+		MMAL_PARAMETER_JPEG_Q_FACTOR, &ctrl_set_image_encode_output
 	},
 };
 
