From 7bb26b1691166d0d830c42c1a25caf82208bf90d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 20 Jun 2014 07:56:40 +0200
Subject: [PATCH] MIPS: BCM47xx: Fix LEDs on WRT54GS V1.0
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Reported-by: Catalin Patulea <cat@vv.carleton.ca>
Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Acked-by: Hauke Mehrtens <hauke@hauke-m.de>
Cc: linux-mips@linux-mips.org
Cc: Hauke Mehrtens <hauke@hauke-m.de>
Patchwork: https://patchwork.linux-mips.org/patch/7113/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/bcm47xx/leds.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/mips/bcm47xx/leds.c
+++ b/arch/mips/bcm47xx/leds.c
@@ -311,6 +311,14 @@ bcm47xx_leds_linksys_wrt54g3gv2[] __init
 	BCM47XX_GPIO_LED(3, "blue", "3g", 0, LEDS_GPIO_DEFSTATE_OFF),
 };
 
+/* Verified on: WRT54GS V1.0 */
+static const struct gpio_led
+bcm47xx_leds_linksys_wrt54g_type_0101[] __initconst = {
+	BCM47XX_GPIO_LED(0, "green", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(1, "green", "power", 0, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(7, "green", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
+};
+
 static const struct gpio_led
 bcm47xx_leds_linksys_wrt610nv1[] __initconst = {
 	BCM47XX_GPIO_LED(0, "unk", "usb",  1, LEDS_GPIO_DEFSTATE_OFF),
@@ -557,6 +565,8 @@ void __init bcm47xx_leds_register(void)
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g3gv2);
 		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0101:
+		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g_type_0101);
+		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0467:
 	case BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0708:
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g_generic);
