From 1aab93c5c97c55fef130726a6f58c9a1fd5b6240 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Tue, 3 Dec 2013 13:36:45 +0100
Subject: [PATCH 4/8] MIPS: BCM63XX: remove !RUNTIME_DETECT code from gpio

---
 arch/mips/bcm63xx/gpio.c | 14 --------------
 1 file changed, 14 deletions(-)

--- a/arch/mips/bcm63xx/gpio.c
+++ b/arch/mips/bcm63xx/gpio.c
@@ -18,19 +18,6 @@
 #include <bcm63xx_io.h>
 #include <bcm63xx_regs.h>
 
-#ifndef BCMCPU_RUNTIME_DETECT
-#define gpio_out_low_reg	GPIO_DATA_LO_REG
-#ifdef CONFIG_BCM63XX_CPU_6345
-#ifdef gpio_out_low_reg
-#undef gpio_out_low_reg
-#define gpio_out_low_reg	GPIO_DATA_LO_REG_6345
-#endif /* gpio_out_low_reg */
-#endif /* CONFIG_BCM63XX_CPU_6345 */
-
-static inline void bcm63xx_gpio_out_low_reg_init(void)
-{
-}
-#else /* ! BCMCPU_RUNTIME_DETECT */
 static u32 gpio_out_low_reg;
 
 static void bcm63xx_gpio_out_low_reg_init(void)
@@ -44,7 +31,6 @@ static void bcm63xx_gpio_out_low_reg_ini
 		break;
 	}
 }
-#endif /* ! BCMCPU_RUNTIME_DETECT */
 
 static DEFINE_SPINLOCK(bcm63xx_gpio_lock);
 static u32 gpio_out_low, gpio_out_high;
