/*
 * Copyright 2013 Freescale Semiconductor, Inc.
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
#include "imx25.dtsi"

/ {
	model = "Freescale i.MX25 Product Development Kit";
	compatible = "fsl,imx25-pdk", "fsl,imx25";

	memory {
		reg = <0x80000000 0x4000000>;
	};
};

&uart1 {
	status = "okay";
};

&fec {
	phy-mode = "rmii";
	status = "okay";
};

&nfc {
	nand-on-flash-bbt;
	status = "okay";
};
