/*
 * Device Tree Source for the sh7372 SoC
 *
 * Copyright (C) 2012 Renesas Solutions Corp.
 *
 * This file is licensed under the terms of the GNU General Public License
 * version 2.  This program is licensed "as is" without any warranty of any
 * kind, whether express or implied.
 */

/include/ "skeleton.dtsi"

/ {
	compatible = "renesas,sh7372";

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "arm,cortex-a8";
			device_type = "cpu";
			reg = <0x0>;
		};
	};

	pfc: pfc@e6050000 {
		compatible = "renesas,pfc-sh7372";
		reg = <0xe6050000 0x8000>,
		      <0xe605801c 0x1c>;
		gpio-controller;
		#gpio-cells = <2>;
	};
};
